Maintain an M60 Machine Gun Reviews
Lubricate the M60 Machine Gun
28 of 44
&pageText=After inspection, the weapon is ready to reassemble, but before you begin assembly, you must properly lubricate the machine gun. To properly lubricate the M60 machine gun:& &label1=Avoid buffer assembly and gas cylinder& &label2=Run patch through bore& &label3=Wipe down non-plastic surfaces& &label4=Lubricate with CLP& &pageNote=Note: When lubricating the M60 machine gun at temperatures below zero degrees Fahrenheit, use LAW and lubricate lightly to avoid freeze-ups. Under all other conditions, use CLP.& &popText1=Do not get CLP inside buffer assembly or gas cylinder.& &popText2=Run cleaning swab dampened with CLP through the bore.& &popText3=Wipe down all non-rubber-coated exterior surfaces with a rag dampened with CLP.& &popText4=Use CLP to lubricate bolt locking lugs by the camming surfaces, operating rod surfaces along receiver rails, actuator roller on bolt, and where bolt actuator rides feed pawl carrier.&