Maintain an M60 Machine Gun Reviews
Remove Buffer, Operating Rod, and Bolt Assembly Group 1
14 of 44
&pageText=There are two parts to removing the buffer, operating rod, and bolt assembly group from the M60. The first
part is to remove the buffer. To do this, you must:& &label1=Apply pressure to rear of buffer& &label2=Remove buffer yoke& &label3=Remove buffer& &label4=Pull buffer plunger from driving spring guide& &label5=Remove driving spring guide and spring& &label6=Separate driving spring from guide& &popText1=Use the palm of your hand to apply slight pressure to the rear of the buffer.& &popText2=Remove the buffer yoke from the top of the receiver.& &popText3=Remove the buffer and allow the driving spring guide to expand until the end of the guide shows at the rear of the receiver.& &popText4=Pull the buffer plunger from the driving spring guide.& &popText5=Pull the driving spring guide and spring from the receiver.& &popText6=Separate the driving spring from the driving spring guide.&