Maintain an M60 Machine Gun Reviews
Clean the M60 Machine Gun
22 of 44
&pageText=Once you have the weapon disassembled, you are able to perform other maintenance procedures such as cleaning the M60. To clean the M60, you must:& &label1=Position gas cylinder& &label2=Clean bore& &label3=Clean chamber& &label4=Clean receiver& &label5=Clean buffer and operating rod group& &label6=Wipe all non-plastic parts& &label7=Dry all parts cleaned with CLP& &warningLabel=Caution:& &warningText=Do not use gasoline, kerosene, benzene, or high pressure water, steam, or air for cleaning the M60.& &popText= & &popText1=Position gas cylinder above barrel to avoid getting CLP in the cylinder.& &popText2=Clean the bore using bore brush and CLP. Do not reverse direction inside bore. Swab bore using a swab and CLP. Swab bore again with dry swab.& &popText3=Clean chamber using chamber brush and CLP. Swab chamber using a swab and CLP. Swab chamber again with dry swab.& &popText4=Clean receiver using receiver brush and CLP. Brush the receiver to remove powder fouling. Swab receiver with a swab and CLP. Swab receiver again with dry swab.& &popText5=Clean buffer and operating rod group using receiver brush and CLP. Brush buffer group to remove powder fouling. Wipe operating rod with a swab or cleaning rag dampened with CLP. Wipe operating rod again with dry swab or cleaning rag.& &popText6=Wipe down all metal parts with a rag and CLP, which will damage rubber or plastic parts. & &popText7=Dry all parts using a clean, dry rag.&