Maintain an M60 Machine Gun Reviews
Replace the M60 Trigger Mechanism Group
35 of 44
&pageText=To replace the M60 trigger mechanism group, you must:& &bulletText1=Engage holding notch& &bulletText2=Rotate mechanism up& &bulletText3=Align mechanism& &bulletText4=Insert retaining pin& &bulletText5=Attach leaf spring& &bulletText6=Engage leaf spring& &popText=& &popText1=Engage the holding notch of the trigger mechanism group into its recess in the bottom of the receiver.& &popText2=Rotate the trigger mechanism up so the top of the mechanism is flush with the bottom of the receiver.& &popText3=Align the holes of the trigger mechanism with the mounting bracket on the receiver.& &popText4=Insert the retaining pin from the left side.& &popText5=Place the open end of the leaf spring onto the retaining pin.& &popText6=Engage the hooked end of the leaf spring onto the sear pin.&