Maintain an M60 Machine Gun Reviews
Replace the M60 Bolt and Operating Rod Assembly
36 of 44
&pageText=To replace the M60 bolt and operating rod assembly, you must:& &bulletText1=Position bolt& &bulletText2=Position operating rod yoke& &bulletText3=Compress firing pin spring& &bulletText4=Seat operating rod yoke& &bulletText5=Push forward on rear of bolt& &bulletText6=Insert operating rod and bolt into receiver& &bulletText7=Insert driver spring guide into driver spring& &bulletText8=Insert driver spring& &bulletText9=Pull trigger& &bulletText10=Push in driver spring& &popText=& &popText1=Hold the bolt in one hand with the camming slot up and the face of the bolt toward your body.& &popText2=With your other hand, position the rear of the operating rod yoke against the firing pin spool.& &popText3=Push the spool forward to compress the firing pin spring.& &popText4=Seat the yoke between the firing pin spool, and allow the yoke to slide back in the bolt assembly.& &popText5=Push forward on the rear of the bolt, so the bolt rotates until the locking lugs are vertical and the cam roller is up.& &popText6=Push the operating rod and bolt into the receiver until the end of the operating rod is even with the rear of the receiver.& &popText7=Insert the driving spring guide into the driving spring.& &popText8=Insert the free end of the driving spring into the opening of the operating rod.& &popText9=Pull and hold the trigger.& &popText10=Push the driving spring until the head of the guide is about one inch from the receiver.&