Maintain an M60 Machine Gun Reviews
Remove Trigger Mechanism Group
16 of 44
&pageText=To properly remove the trigger mechanism group, you must:& &bulletText1=Press leaf spring& &bulletText2=Rotate leaf spring& &bulletText3=Disengage leaf spring& &bulletText4=Remove retaining pin& &bulletText5=Remove trigger mechanism& &popText1=Press in on the rear of the leaf spring.& &popText2=Rotate the rear of the leaf spring upward to clear it from the sear pin.& &popText3=Pull the leaf spring to the rear, disengaging it from the front notch of the retaining pin.& &popText4=Remove the retaining pin by pushing it to the left.& &popText5=Slide the trigger mechanism forward, rotate the front downward, and remove the mechanism from the receiver.&