Maintain an M249 Machine Gun Reviews
Summary – Perform a Function Check
53 of 54
&pageText=To correctly perform a function check on the M249 machine gun, you must:& &bulletText1=Grasp the cocking handle and pull bolt to the rear& &bulletText2=Move the safety to the SAFE position& &bulletText3=Push the cocking handle to the forward position& &bulletText4=Pull the trigger& &bulletText5=Grasp the cocking handle and pull and hold it to the rear& &bulletText6=Move the safety to the FIRE position& &bulletText7=Pull the trigger while riding the bolt forward& &bulletTime1=12000& &bulletTime2=15800& &bulletTime3=18700& &bulletTime4=22400& &bulletTime5=24500& &bulletTime6=28700& &bulletTime7=32000& &numBullets=7& &timedText=true& &audioXpos=350& &audioYpos=10& &textPosition=left&