Maintain an M249 Machine Gun Reviews
Summary – Inspect for Serviceability
35 of 54
&pageText=To correctly inspect the M249 machine gun for serviceability, you must complete the serviceability checks for each of the eight major groups:& &bulletText1=Operating rod group& &bulletText2=Barrel group& &bulletText3=Handguard group& &bulletText4=Buttstock and buffer assembly group& &bulletText5=Trigger mechanism group& &bulletText6=Gas cylinder group& &bulletText7=Bipod group& &bulletText8=Receiver group& &bulletTime1=22000& &bulletTime2=23800& &bulletTime3=25400& &bulletTime4=26800& &bulletTime5=28800& &bulletTime6=30600& &bulletTime7=32800& &bulletTime8=34400& &numBullets=8& &timedText=true& &audioXpos=315& &audioYpos=75&