Maintain an M249 Machine Gun Exercises
Summary
12 of 12
&scoringAreas=7& &label0=Cleared the M249 machine gun.& &label1=Disassemble the M249 machine gun.& &label2=Clean the M249 machine gun.& &label3=Inspect the M249 machine gun.& &label4=Lubricate the M249 machine gun.& &label5=Assemble the M249 machine gun.& &label6=Perform a function check to ensure you have assembled the weapon correctly.& &nogo0=Failure to clear the M249 machine gun results in an unsafe condition for the gunner and those soldiers nearby.& &nogo1=Failure to disassemble the M249 machine gun results in the weapon not being able to be properly cleaned, inspected for serviceability and lubricated.& &nogo2=Failure to clean the M249 machine gun results in the weapon not operating correctly when being fired.& &nogo3=Failure to inspect the M249 machine gun results in the weapon becoming unserviceable or potentially dangerous to operate.& &nogo4=Failure to lubricate the M249 machine gun results in the weapon not operating correctly when being fired.& &nogo5=Failure to assemble the M249 machine gun results in the weapon not firing properly and presenting an unsafe situation for the gunner and those soldiers nearby.& &nogo6=Failure to perform a function check on the M249 machine gun results in the gunner not knowing whether the weapon will function correctly and presents an unsafe situation for the gunner and those soldiers nearby.& &sequence=true& &sequenceLabel=Completed tasks in the correct sequence.& &gotext=You have completed this exercise correctly. Click the Options button, select exit and then select another task.& &nogotext=You did not complete this exercise successfully. Click the Options button, select Exit, and then select Maintain an M249 Machine Gun to review this material.&