Maintain an M249 Machine Gun Reviews
Summary – Lubricate the Machine Gun
39 of 54
&pageText=To correctly lubricate the M249 machine gun, you must accomplish the following procedures:& &bulletText1=Cover all metal surfaces of the machine gun, with a light coat of CLP, to include:
◦ Operating rod group
◦ Barrel group
◦ Receiver group& &bulletText2=A light coat is defined as a film barely visible to the eye.& &bulletText3=CLP is the only lubricant authorized for this weapon.& &bulletTime1=18300& &bulletTime2=27400& &bulletTime3=32000& &numBullets=3& &timedText=true& &textPosition=left& &audioXpos=370& &audioYpos=20&