RAD Studio |  |

disable, _disable, enable, _enable

Header File

dos.h

Category

Miscellaneous Routines

Prototype

void disable(void);

void _disable(void);

void enable(void);

void _enable(void);

Description

Disables and enables interrupts.

These macros are designed to provide a programmer with flexible hardware interrupt control.

disable and _disable macros disable interrupts. Only the NMI (non-maskable interrupt) is allowed from any external device.

enable and _enable macros enable interrupts, allowing any device interrupts to occur.

Return Value

None.

Portability

POSIX | Win32 | ANSI C | ANSI C++
| + |  |

Copyright(C) 2009 Embarcadero Technologies, Inc. All Rights Reserved.
What do you think about this topic? Send feedback!