30/30

# Index

A B C D E F G H I J K L M N O P Q R S T U V W

## A

  AC breaker panels, 2.4.2
  AC power, location, 2.4.2
  access route requirements, 2.2.1, 2.2.1
  accessing servers from KVM, 7.1.5
  accessory kits, 1.4
  acoustic levels, 2.1, 2.1
  add subcommand (Mammoth Reconfiguration Utility), 10.12
  adding racks, 10.5
  adding services, 13
  adding to an existing cluster configuration options, 4.15.1
  administration software overview, 1.5
  administrative network, 3.1.2
    cabling requirements, 2.7
    connections, 2.7
    ports, 3.1
  administrative network diagram, 15.2
  Administrative Network page (configuration), 4.10
  administrative utilities, 1.5
  African PDU specifications, 2.4.1.4
  air conditioning, 2.5, 2.8, 6.1
  airflow, 2.1, 2.1, 2.5
  airflow requirements, 2.6
  alert notifications, 4.15.3.9
  alerts, 15.1, A.1
  Allen wrench keys, 6.3.2.2
  altitude requirements, 2.5
  ambient relative humidity range, 2.5
  ambient temperature range, 2.5, 11.1
  American PDU specifications, 2.4.1.1, 2.4.1.2
  Asia Pacific PDU specifications, 2.4.1.4
  ASR
    about, 5.1
    activating assets, 5.6
    adding support, 10.8.2, 10.12
    configuration, 5.2
    installation prerequisites, 10.2
    troubleshooting, 5.8
    validation, 5.7, 10.4.1
  ASR Manager, 4.15.3.7
    installation, 5.3
    port number, 4.15.3.7
  ASR network connections, 5.2
  ASR trap destinations, 5.5
  asrexacheck script, 10.4.1
  asset verification (ASR), 5.6
  Audit Vault
    installation prerequisites, 10.2
    plug-in configuration, 4.15.3.6
  Auto Service Request
    alerts, A.1
    configuration, 4.15.3.7
    installing, 10.11.2
    port assignments, 3.4
    See also ASR

## B

  base image files, 10.3
  base image reinstallation, 10.9
  base image utilities, 10.13.1
  batteries
    life expectancy, B.2
    replacement policy, B.2
  BDA server offline repair category, B.1
  BDA_REBOOT files, 6.4.3, 13
  bda_reboot_status file, 13
  bdacheckcluster utility, 13
  bdacheckhw utility, 7.5, 11.5.3, 13
  bdacheckib utility, 13
  bda-checkip.out file, 3.5
  bdachecknet utility, 8.4.3, 13
  bdachecksw utility, 7.5, 11.5.3, 13
  bdacli utility, 13
  bdaclustersynctime utility, 13
  BdaDeploy.json configuration file, 10.9.2
  BdaDeploy.json file, 4.3, 4.3, 7.6
  bdadiag utility, 13
  BdaExpansion.json file, 4.3, 4.3, 8.4.1
  bdagetclientconfig utility, 13
  bdaid utility, 13
  bdaimagevalidate utility, 13
  bda-install-review.html file, 4.3
  BDAMammoth directory, 10.11, 10.12
  BDA-O repair category, B.1
  bda-preinstall-checkip.sh file, 4.3
  bdaredoclientnet utility, 13
  bdaserials utility, 13
  bdaswapoff utility, 13
  bdaswapon utility, 13
  bdaupdatefw utility, 13
  bda.zip configuration archive, 4.3
  Big Data Appliance
    See Oracle Big Data Appliance
  Big Data Connectors
    See Oracle Big Data Connectors
  Big Data SQL
    starting, stopping, restarting, 13
  black cables, 1.4, C.1, D.1
  blue cables, 1.4, C.1, D.1
  bolts, 6.3.2.2
  bondeth0 interface
    network connections, 3.1.1
  bondib0 interface
    description, 3.1.2
    maintenance, 11.5
  bondib0 network
    verifying operations, 11.5.3
  boot order, resetting, 13
  breaker panels, 2.4.3

## C

  cable tie,
    removing, 6.4.2
  cable-routing floor cutout, 6.3.2.2
  cables, 1.4
    color coding, C.1, D.1
    spare parts, 1.4
    spares, 1.4
    splitter, 3.2.2
  cabling
    client network, 3.2
    eight racks, E.9
    existing network requirements, 2.7
    five racks, E.6
    four racks, E.5
    multirack, 9.3, E.1
    seven racks, E.8
    six racks, E.7
    spare parts, B.9
    three racks, E.4
    two racks, E.3
  cabling tables
    with KVM (Sun Fire servers), D
    without KVM (X4-2L and X3-2L servers), C
  cage nuts, 6.2.1
  casters, 6.3.1
  cautions, 11.2.3
  CDH
    health checks, 13
  CDH cluster configuration, 4.15.3, 10.5
  CDH cluster logs, 13
  CDH installation, 10.11.2
  CDH ports, 3.4
  CDH services, starting, 10.11.2
  ceiling height requirements, 2.2
  checking firmware, 7.5, 7.5
  checking network configuration, 13
  checking the server software, 13
  circuit breakers, 2.4.3, 2.4.3, 6.4.3
  Cisco switch
    replacement parts, B.7
    See Ethernet switch
  CleanupInstall step, 10.11.2
  CleanupSSHroot step, 10.11.2
  CLI utility, 13
  CLI, Oracle ILOM, 15.1.1
  client access network
    cabling requirements, 2.7
    description, 3.1.2
    requirements, 2.7
  client configuration distribution, 13
  Client Ethernet Network page (configuration), 4.9
  client network
    bandwidth, 3.2.1
    cabling, 3.2
    configuration, 4.7
    traffic routing through switches, 3.2.1
  client network connections, 3.2.5
  clock configuration
    Ethernet switch, 7.2.6
    InfiniBand switches, 7.3.2
  Cloud Control, 1.5
    See Also Oracle Enterprise Manager Cloud Control
    See also Oracle Enterprise Manager
  Cloudera’s Distribution including Apache Hadoop
    See CDH
  cluster expansion, 10.5
  cluster name configuration, 4.14
  cluster naming conventions, 4.5.3
  Cluster page (configuration), 4.15
  cluster reimaging, 10.13.2
  cluster_name-config.json, 4.3
  cmf.keytab file, 10.2
  collecting diagnostics, 13
  color coding, cables, C.1, D.1
  command files, executing across servers, 14.2
  command-line interface, 13
  commands, remote execution across servers, 1.5, 14
  Complete page, 4.16
  component configuration, full or starter rack, 7
  component failure, environmental causes, 2.5
  component names, 4.5.4
  components
    location in the rack, C.2, D.2
    server, 1.3
    spare parts kit, 1.4
  configuration
    disk controller, 11.4.1.1
    editing in the Configuration Generation utility, 4.2
    full or starter rack components, 7
    in-rack expansion kit, 8
    physical drives, 11.4.1.3
    querying, 13
    virtual drive, 11.4.1.2
  configuration files, 4.3
    copying to new servers, 8.4.1
    generating, 4.2, 4.16
    ntp.conf file, 11.7
  Configuration Generation Utility
    input file, 4.3
    installing, 4.2
    overview, 4.1
  configuration worksheets
    See Configuration Generation Utility
  configure terminal command, 7.2.3
  configuring a new disk, 12.5
  configuring ASR, 5.2
  configuring Ethernet switch, 7.2, 7.2.3
  configuring KVM, 7.1, 7.1.4
  configuring servers, 7.5
  connecting KVM to the network, 7.1.2
  connectors
    See Oracle Big Data Connectors
  cooling requirements, 2.1, 2.1
  copper cables, 1.4
  copying files, 14.1.1
  CopyLicenseFiles step, 10.11.2
  CopySoftwareSource step, 10.11.2
  corrosion problems, 2.5
  CreateLogicalVolumes step, 10.11.2
  CreateUsers step, 10.11.2
  Customer Details Page (configuration), 4.5

## D

  data center switch configuration, 2.8
  dba group, 4.15.3.1, 10.11.2
  dcli utility
    description, 1.5
    examples, 14.4
    option descriptions, 14.2
    return values, 14.3
    syntax, 14.2
    target servers, 14.1.2.2
    using, 14
  Define Clusters page (configuration), 4.14
  diagnostics collection, 13
  dimensions
    rack, 2.2
    shipping, 2.2.1
  DIMM slots, adding memory, 11.3.1
  directories, copying files across servers, 14.2
  disablesm command, 7.3.3, 9.3, 9.4, 9.4, 11.5.2
  disk controllers, 11.4.1, 11.4.1.1
  disk drives
    physical slots, 12.2.1
    server status indicators, B.3.1
    spares, 1.4, B.4
    symbolic links, 12.2.1
  disks
    configuring, 12.5
    repairing, 11.4
    replacing, 12
  DNS network registration, 2.8
  DNS server requirement, 3.1.2, 3.1.2, 4.12
  documentation, third-party hardware, 1.4
  domain name system configuration, 4.12
  door dimensions, 2.2.1
  downgrading the factory image, 10.5
  drive configuration, physical, 11.4.1.3

## E

  earth ground cable, 6.3.3
  electric receptacles, 2.4.1
  electrical access, 2.2.2
  electrical requirements, 2.4, 6.1, 6.4.3
  electrical storms, 2.4
  electronic noise, 6.1
  electrostatic discharge, 2.5
  elevator requirements, 2.2.1
  email accounts
    alerts (Cloudera Manager), 4.15.3.9
  email accounts, My Oracle Support (ASR), 5.1
  email alerts configuration, 4.15.3.9
  emergency shutdown, 11.2.2
  enablesm command, 7.3.3, 9.3, 9.4, 9.4
  encryption, 10.8.5
    adding support, 10.12
  engineered systems, connecting to Oracle Big Data Appliance, C.7, D.8
  Enterprise Management Cloud Control configuration, 4.15.3.8
  Enterprise Manager
    See Also Oracle Enterprise Manager Cloud Control
  env_test command, 7.3.3
  environmental requirements
    full rack, 2.1
    starter rack and expansion kit, 2.1
  environmental specifications, 2.1, 2.1
  error messages, A.1
  eth0 interface, 3.1.2
  Ethernet bridge ports, 13
  Ethernet cabling, 2.7, 3.2.1
  Ethernet interface, 3.1.2
  Ethernet over InfiniBand protocol., 3.2.1
  Ethernet ports, 2.1, 2.1, 3.1
  Ethernet switch
    configuration, 7.2, 7.2.2
    configuring host name, 7.2.3
    IP routing, 7.2.3
    port speed, 7.2.3
    replacement parts, B.7
    replacement switch, 1.6
    setting remote password, 7.2.4
    spare parts, 1.4
    time settings, 7.2.6
    validating and saving configuration, 7.2.9
  European PDU specifications, 2.4.1.4
  expansion kit
    See in-rack expansion kit
  ext4 file system, 12.8.3
  external filer configuration, 10.11.2

## F

  Fabric Management, 7.3.3
  factory image reinstallation, 10.9
  factory patches, 10.11.2
  failover connections, 3.1.1, 3.1.1, 3.1.2, 3.2.1
  fan modules
    server status indicators, B.3.1
    switch status indicators, B.3.2
  Fibre Channel over Ethernet, 1.6
  files, copying to multiple servers, 14.2
  filler panels, 2.6
  firewall configuration, 2.8
  Firmware State status, 12.5
  firmware updates, 13
  firmware upgrades
    KVM switch, 7.1.3
    restrictions, 1.6
  first server location, 7.6.1
  floor cut dimensions, 6.3.2.2
  floor load, 2.2.1, 2.3, 2.3
  floor tiles, 2.6
  flooring
    raised, 2.3
    raised pattern, 2.2.1
  Foreign State status, 12.5
  forklift, 2.2.1
  FRUs, B
  full rack component configuration, 7

## G

  gateway configuration
    Ethernet switch, 7.2.3
  gateway switch factory IP addresses, 3.3
  gateway switch ports, D.8
  gateway switches
    assigning to VNICs, 3.2.1
    cabling, 3.2
    configuring, 7.3
    connecting to Oracle ILOM, 15.5.2
    guidelines for connecting, 3.2.4
    replacing, 11.5.2
    using splitter cables, 3.2.2
    See also InfiniBand switches
  General Network Properties page (configuration), 4.12
  getmaster command, 9.3, 9.4, 9.4
  getting help, 13
  ground cable, 6.3.3, 6.3.3
  grounding resistance, 6.1
  grounding to earth, 2.4.3
  groups, hadoop, 10.11.2
  GRUB master boot records, 12.8.5

## H

  Hadoop cluster configuration, 4.15.3, 10.5
  hadoop group, 10.11.2
  Hadoop installation, 10.11.2
  Hadoop ports, 3.4
  Hadoop services, starting, 10.11.2
  hardware configuration, 4.6
    querying, 13
  hardware diagnostics, 15
  hardware failures, automatic reporting, 5.1
  hardware profiles, acquiring from servers, 7.5
  Hardware Selection page (configuration), 4.6
  hardware status indicators, B.3
  hardware validation, 13, 13, 13
  HDFS diagnostics, 13
  HDFS disk formatting, 12.9
  HDFS partitions, 12.2.2
  hdfs user, 10.11.2
  health checks on InfiniBand switches, 7.3.3
  high-voltage PDUs, 2.4.1.4, 11.8, 11.8
  host factory IP addresses, 3.3
  hot swap repair category, B.1
  HS repair category, B.1
  humidity range, 2.5, 2.5

## I

  ibdiagnet utility, 11.5.3
  iblinkinfo utility, 13
  ibqueryerrors utility, 11.5.3
  ibstatus utility, 7.5
  ILOM
    See Oracle ILOM
  ilom-admin default password, 7.3.1
  ilom-admin user, 15.1.2
  ilom-operator user, 15.1.2
  image validation, 13
  image version
    downgrading, 10.5
    upgrading, 10.5
  imagehistory utility, 13
  imageinfo utility, 10.5, 13
  incline, maximum, 2.2.1
  InfiniBand configuration, 7.3
  InfiniBand Gateway switch ports, D.8
  InfiniBand network
    cabling checks, 13
    factory IP addresses, 3.3
  InfiniBand network interface card, 3.1
  InfiniBand Network page (configuration), 4.11
  InfiniBand network verification, 11.5.3
  InfiniBand ports, connecting to other devices, C.7, D.8
  InfiniBand private network, 3.1.2
  InfiniBand Subnet Manager, 11.5.4
  InfiniBand switches
    checking status, 7.5
    configuring, 7.3
    health checks, 7.3.3
    priority settings, 7.3.3
    replacing, 11.5.2
    setting time zone, 7.3.2
    spare parts, B.5, B.6
  infrastructure repair category, B.1
  in-rack expansion kit
    cables, 8.1.1
    components, 8.1.1
    configuration, 8
    configuring servers, 8.3
    installing servers, 8.2
    network configuration, 8.4.2
    PDU firmware requirement, 8.1.2
  installation of in-rack expansion kit, 8.2
  installation policy for third-party software, 1.6
  installation prerequisites, 10.2
  InstallBDASoftware step, 10.11.2
  InstallHadoop step, 10.11.2
  installing base image, 10.9
  installing patches, 10.11.2
  installing the software
    See also Mammoth Utility
  International Electrotechnical Commission (IEC), 2.4.4
  IP address requirements, 2.1, 2.1
  IP addresses
    administrative network configuration, 4.10
    client network configuration, 4.9
    editing individual, 4.13
    factory settings, 3.3
    InfiniBand network configuration, 4.11
  IP routing, 7.2.3
  ipmitool command, 7.5
  IR repair category, B.1

## J

  Japanese PDU specifications, 2.4.1.1, 2.4.1.2
  jumper brackets, 6.2.1

## K

  Kerberos authentication
    adding support, 10.8.6, 10.12
    configuration, 4.15.3.4
    installation prerequisites (remote KDC only), 10.2
  Kerberos configuration, 10.11.2
  kernel device names (disk drives), 12.2
  key distribution center, 4.15.3.4, 10.2
  KVM switch
    accessing servers, 7.1.4
    cabling, D.3
    configuration procedures, 7.1
    connecting to the network, 7.1.2
    firmware upgrades, 7.1.3
    MAC address, 7.1.2
    naming, 7.1.2
    starting, 7.1.1

## L

  leaf switches
    configuring, 7.3
    See also InfiniBand switches
  LED color codes, B.3.1, B.3.2
  LED status indicators, B.3
  leveling bolts, 6.2.2
  leveling feet, 6.3.1, 6.3.2.1
  license location, 10.11.2
  licensing restrictions, 1.6
  lift gate, 2.2.1
  lightning arresters, 2.4
  lights-out management, 15
  listlinkup command, 13
  loading dock, 2.2.1
  locating first server, 7.6.1
  locks, panel, 6.2.1
  low-voltage PDUs, 2.4.1.1, 2.4.1.2, 11.8, 11.8

## M

  MAC address of KVM switch, 7.1.2
  MAC addresses, 13
  maintenance access requirements, 2.2.2
  makebdaimage utility, 10.13.1
  Mammoth download, 10.3
  Mammoth installation files, 10.3
  Mammoth options, 10.11.1
  Mammoth Reconfiguration Utility, 10.12
  Mammoth Utility
    description, 10.4
    execution steps, 10.11.2
    location, 10.11
    reasons for failure, 10.5
    running, 10.4.1
    synchronizing clocks, 7.3.2
    syntax, 10.11, 10.11
  mammoth-rack_name.params file, 4.3
  management network
    cabling requirements, 2.7
    connecting the KVM, 7.1.2
    connections, 2.7
    factory IP addresses, 3.3
    ports, 3.1
  management utilities, 1.5, 1.5, 15.1.1
  mapred user, 10.11.2
  master.xml configuration file, 4.3
  MegaCli64 command, 7.5, 11.4.1.1
  memory, adding to servers, 11.3
  Middle Eastern PDU specifications, 2.4.1.4
  minimum ceiling height, 2.2
  monitoring PDUs, 11.8
  mount points, 12.2.2
  mount_hadoop_dirs utility, 13
  mounting a device, 7.6.1
  mounting brackets, 6.2.2, 6.3.2.2, 6.3.2.2
  mounting tool, 6.2.1
  multirack cabling
    procedures, 9.1
    three to eight, 9.4
    two racks, 9.3
  multirack clusters, 3.2.5
  multirack software configuration, 10.5
  My Oracle Support email account, 5.1
  MySQL Database installation, 10.11.2

## N

  naming conventions, 4.5.4
  NET0, 3.1.2
  network
    connecting the KVM, 7.1.2
    factory IP addresses, 3.3
  network configuration, 4.8
  network configuration file, 4.3
  network connections, 2.7, 7.6.3
    ASR, 5.2
    reconfiguring 10GbE, 13
  network diagrams, 3.1.3, 3.1.3, 15.2
  network errors, checking for, 3.5
  network interfaces, InfiniBand card, 3.1
  network operations, verifying InfiniBand, 11.5.3
  network registration, 2.8
  network requirements, 2.1, 2.1
  network settings
    preinstall validation, 4.4
  network suffix configuration, 4.5
  network time protocol, 4.12, 11.7
  network topology, 11.5.4
  network validation, 13, 13
  Networking page (configuration), 4.8
  networks
    administrative, 3.1.2
    client access, 2.7, 3.1.2
    descriptions, 3.1.2
    InfiniBand, 3.1.2
  networksetup scripts, 7.6.2, 7.6.5
  networksetup-one script, 8.4.2
  networksetup-two script, 8.4.2
  noise, electronic, 6.1
  North American PDU specifications, 2.4.1.1, 2.4.1.2
  NTP server requirement, 3.1.2, 3.1.2, 4.12
  NTP servers, 11.7
    configuring, 7.2.7
    setting on InfiniBand switches, 7.3.2
  ntp.conf file, 11.7
  nuts, 6.2.1

## O

  ODI
    See Oracle Data Integrator
  oinstall group, 4.15.3.1, 10.11.2
  on-disk encryption, 10.8.5
  operating cautions and warnings, 11.2.3
  operating system disks, 12.8, 12.8
  operating system history, 13
  operating system image, 13
  Oracle Audit Vault and Database Firewall
    plug-in configuration, 4.15.3.6
    See also Audit Vault
  Oracle Big Data Appliance
    general description, 1.1
    rack components, 1.2
    server components, 1.3
  Oracle Big Data Connectors
    configuration, 4.15.3.3
    installation, 10.5, 10.11.2
    installing server components, 4.15.3.3
    software installation, 10.5
  Oracle Data Integrator, 4.15.3.3
  Oracle Enterprise Manager
    adding support, 10.12
    troubleshooting, 10.2
  Oracle Enterprise Manager agent installation, 10.11.2
  Oracle Enterprise Manager Cloud Control, 1.5, 4.15.3.8
    adding support on Oracle Big Data Appliance, 10.8.3
    rediscovery, 10.5
    See also Oracle Enterprise Manager
  Oracle Enterprise Manager plug-in installation prerequisites, 10.2
  Oracle Exadata Database Machine, 4.15.3.1
  Oracle ILOM, 15
    backing up configuration, 11.5.1.1
    connecting to CLI, 15.4.1
    connecting to web interface, 15.4.2
    description, 15.1
    Ethernet connections, 15.4
    factory IP addresses, 3.3
    opening serial connections, 15.5
    restoring configuration, 11.5.1.2
    user interfaces, 15.1.1
  Oracle ILOM port, 3.1
  Oracle Inventory Group, 4.15.3.1
  Oracle Linux, 1.1
  Oracle NoSQL Database
    configuration, 4.15.2, 4.15.2.1
    creating logical volumes, 10.11.2
    disk formatting, 12.9
    installation, 10.11.2
  Oracle Support, 13
  oracle user name, 4.15.3.1
  orange cables, 1.4, C.1, D.1
  OS watcher logs, 13

## P

  pallet jack, 2.2.1
  panel locks, 6.2.1
  parallel execution of commands, 14
  partitions
    creating on a new disk, 12.8.1.1, 12.8.1.2
    dismounting, 12.3
  parts kit, 1.4
  passwordless SSH, 13, 13, 14.1.1
  passwords (default)
    Ethernet switch, 7.2.3
    ilom-admin, 7.3.1
    PDU metering unit, 7.4.1
    servers, 7.5
  patch installation, 10.11.2
  PatchFactoryImage step, 10.11.2
  path to data center, 2.2.1
  PDAs, location in the rack, C.2, D.2
  PDU configuration, 7.4.1
  PDU metering unit password, 7.4.1
  PDU requirements, 2.4.1
  PDU specifications
    for America, Japan, Taiwan, 2.4.1.1
    for Americas, Japan, Taiwan, 2.4.1.2
    for Europe, Middle East, Africa, Asia Pacific, 2.4.1.4
  PDU thresholds, 11.8
  PDUs
    circuit breakers, 6.4.3
    network connections, 7.4.1
    powering on, 6.4.3
    replacement parts, B.8
    single-phase, 6.1, 6.4.3
  perforated tiles, 2.6
  photocopiers, 6.1
  physical drive configuration, 11.4.1.3, 11.4.1.3
  port assignments, 3.4
  port speed of Ethernet switch, 7.2.3
  ports
    ASR Manager, 4.15.3.7
    connecting to 40 GbE, 3.2.3
  ports, open gateway, C.7, D.8
  power connectors, 2.4.1
  power cord length requirements, 2.4.2
  power cords, 2.4.3, 2.4.4
    connecting to rack, 6.4.2
    removing cable ties, 6.4.2
    routing, 6.4.2
  power LED locations, 6.4.3
  power off switch, 11.2.2.1
  power outlet grounding, 2.4.4
  power receptacle location, 2.4.2
  power requirements, 2.1, 2.1, 2.4
  power supplies
    server status indicators, B.3.1
    switch status indicators, B.3.2
    uninterruptable, 2.4.3
  powering off
    emergency, 11.2.2.1
    sequence, 11.2.1.2
  powering on, 6.4.3, 11.2.1.1
  preinstallation tasks, 2.8
  preinstall-checkip script
    running, 3.5
  preinstall-checkip.sh file, 4.3, 4.4
  prerequisites to software installation, 10.2
  private network
    verifying operations, 11.5.3
  problem reporting, 5.1
  Puppet utility, 10.11.2, 10.11.2

## Q

  QSFP cables, 1.4
  QSFP ports, splitting, 3.2.2
  querying configuration, 13

## R

  rack base name configuration, 4.5
  rack components, 1.2
  rack configuration file, 10.5
  Rack Details page (configuration), 4.7
  rack dimensions, 2.2
  rack layout illustration, C.2, D.2
  rack layouts
    with KVM (Sun Fire servers), D.2
    without KVM, C.2
  rack reimaging, 10.9.2
  rack weight, 2.1, 2.1
  racks
    adding another, 9.1
    connecting power cords, 6.4.2
    inspecting, 6.4.1
    installing Oracle Big Data Appliance software, 10.4
    moving instructions, 6.3.1
    reimaging, 10.13.3
    reinstalling base image, 10.9
  RAID arrays, repairing logical, 12.8.2
  RAID configuration, 7.5
  RAID logical drives, 12.2.1
  red cables, 1.4, C.1, D.1
  reimagecluster utility, 10.13.1, 10.13.2
  reimagerack utility, 10.13.1, 10.13.3
  reimaging a rack, 10.9.2
  reimaging the servers, 10.9
  reinstalling the software, 10.4.1
  relative humidity, 2.5, 2.6
  remove-root-ssh script, 13, 14.1.1
  removing services, 13
  repair categories, B.1
  replacement parts, B
  replacing spine switch, 11.5.2
  reset-boot-order utility, 13
  resolv.conf configuration file, 8.4.3
  restart validation, 6.4.3
  restarting Big Data SQL, 13
  restrictions on use, 1.6
  Review and Edit Details page (configuration), 4.13
  root user, passwordless SSH, 14.1.1
  route requirements, 2.2.1
  running-config output, 7.2.9

## S

  safety guidelines, 6.1
  scp file copy utility, 14.1.1
  screwdrivers, 6.2.1
  screws, 6.2.1
  search domain configuration, 4.12
  sensor monitoring, 15.1
  serial numbers, 13
  server boot order, resetting, 13
  server components, 1.3
  server configuration, 7.5
    in-rack expansion kit, 8.3
  server diagnostics, 13
  server disks
    configuring, 12.5
    replacing, 12
  server factory IP addresses, 3.3
  server LEDs, B.3
  server locations in the rack, C.2, D.2
  server software validation, 13
  servers
    adding memory, 11.3
    adding to a cluster, 10.5
    allocating into clusters, 4.14
    connecting to Oracle ILOM, 15.5.1
    default passwords, 7.5
    LED color codes, B.3.1, B.3.2
    location in the rack, C.2, D.2
    monitoring, 15
    spare parts, B.4, B.4
    upgrading base image, 10.9
  service locations, restrictions on moving, 1.6
  services, starting, 10.11.2
  setsmpriority command, 7.3.3, 9.3, 9.4, 9.4
  SetupASR step, 10.11.2
  SetupEMAgent step, 10.11.2
  SetupInstall step, 10.11.2
  SetupKerberos step, 10.11.2
  SetupMountPoints step, 10.11.2
  SetupMySQL step, 10.11.2
  SetupPuppet step, 10.11.2
  setup-root-ssh script, 11.6, 13, 14.1.1
  shipping dimensions, 2.2.1, 6.2
  shipping kit, 6.2.1
  shipping weight, 2.2.1
  show command, 7.2.9
  showunhealthy command, 7.3.3
  showusb utility, 7.6.1, 13
  showvlan utility, 13
  showvnics utility, 13
  shutdown command, 11.2.1.2.1
  single-phase PDUs, 2.4.1.1, 6.1, 6.4.3, 11.8, 11.8
  site readiness tasks, 2.8
  slot numbers (disk drives), 12.2.3
  slots, disk drives, 12.2.1
  SMTP alerts, 5.1
  SNMP alerts, 5.1
  software configuration
    querying, 13
  software image
    downgrading, 10.5
    upgrading, 10.5
  software installation
    multiple racks, 10.5
    upgrading, 10.7
    using Mammoth, 10.4
  software installation policy, 1.6
  software options, adding after installation, 10.12
  software port assignments, 3.4
  software profiles, acquiring from servers, 7.5
  software source code, third party, 10.11.2
  software validation, 13, 13
  sound levels, 2.1, 2.1
  South American PDU specifications, 2.4.1.1, 2.4.1.2
  spares kit, 1.4, 6.2.2
  spine switches
    cabling, E.1.3
    configuring, 7.3
    replacing, 11.5.2, 11.5.2
  splitter cables, 3.2.2
  spring nuts, 6.2.1
  SSH
    removing passwordless, 13
    setting up passwordless, 13
  SSH keys, checking rack distribution, 7.5
  stabilizing feet, 6.3.1
  stabilizing the rack, 6.3.2.1, 6.3.2.2
  starter rack
    component configuration, 7
    expanding, 8.1
    physical layout, C.2
  StartHadoopServices step, 10.11.2
  starting KVM, 7.1.1
  starting or stopping Big Data SQL, 13
  startup order, resetting, 13
  state file, 10.5
  static discharges, 2.5
  static electricity, 6.1
  status indicators, B.3
  Subnet Manager, 9.3, 9.4, 11.5.4
  Subnet Manager Master, 9.4
  Subnet Managers, 11.5.4
  subnet mask factory settings, 3.3
  Sun Network 10 GbE Switch 72p, 1.6, 3.2.3
  Sun Network QDR InfiniBand Gateway Switch, 11.6, 13, 13
  Sun Server components, 1.3
  support accounts, 5.2
  support services, 13
  swap partition, restoring, 12.8.4
  swapping, 12.3, 12.3, 13, 13
  switch LEDs, InfiniBand switch LEDs, B.3
  switch ports, D.8
  switches
    location in the rack, C.2, D.2
    monitoring, 15
    naming conventions, 4.5
    replacement parts, B.7
    replacing, 11.5.2
    setting host names, 7.3.1
    spare parts, B.5, B.6
    third-party, 1.6
  symbolic link names (disk drives), 12.2
  synchronizing servers, 13

## T

  Taiwanese PDU specifications, 2.4.1.1, 2.4.1.2
  tee utility, 8.4.2
  telnet access, configuring Ethernet switch, 7.2.4
  temperature
    acceptable range, 2.5
    operating range, 2.5
  test events (ASR), 5.7
  testrule setting (ASR), 5.7
  third-party license location, 10.11.2
  third-party software, 1.6
  third-party software source code, 10.11.2
  third-party switches, restrictions on use, 1.6
  three-phase PDUs, 2.4.1.2, 2.4.1.4, 11.8, 11.8
  thresholds for PDUs, 11.8
  time synchronization, 13
  time zone
    configuration setting, 4.5
    configuring Ethernet switch, 7.2.6
    configuring InfiniBand switches, 7.3.2
    setting summer time, 7.2.6
  top clearance (rack), 2.2
  trap destinations (ASR), 5.5

## U

  unpacking instructions, 6.2.2
  upgrade history, 13
  upgrading base image, 10.9
  upgrading the factory image, 10.5
  upgrading the software, 10.7
  UPS, 2.4.3
  USB devices, restrictions on use, 1.6
  USB flash drive, 7.6.1, 13
  users, hdfs and mapred, 10.11.2

## V

  validating a cluster, 13
  validating hardware and software, 13
  validating network configuration, 13
  validating the server software, 13
  validation checks after reboot, 6.4.3
  ventilation requirements, 2.6, 2.6
  verifying
    database server configuration, 11.4.1
  version command, 7.3.3
  virtual drive configuration, 11.4.1.2
  VLANs
    configuration, 13
    configuration example, 7.2.3
    default configuration, 3.1.1
  VNICs
    assigning to gateway switches, 3.2.1
    configuration, 13
    default configuration, 3.1.1
    re-creating, 13

## W

  warnings, 11.2.3
  warranty restrictions, 1.6
  washers, 6.3.2.2
  watcher logs (OS), 13
  weight
    rack, 2.1, 2.1
    shipping, 2.2.1
  wrenches, 6.2.1, 6.3.2.2
  wrist strap, 6.2.1