28/30

# D In-Rack Cabling Tables for Oracle Big Data Appliance

The tables in this appendix show the in-rack cable connections for Sun Fire X4270 M2-based Oracle Big Data Appliance racks. This appendix contains the following sections:

- Cable Color Coding

- Oracle Big Data Appliance Rack Layout

- KVM Network Cable Connections

- Administrative Gigabit Ethernet Cable Connections

- Oracle Integrated Lights Out Manager Cable Connections

- Single-Phase Power Distribution Unit Cable Connections

- Three-Phase Power Distribution Unit Cable Connections

- In-Rack InfiniBand Switch-to-Switch Cable Connections

- In-Rack InfiniBand Switch-to-Server Cable Connections

## D.1 Cable Color Coding

The cables used in Oracle Big Data Appliance are color-coded as follows:

- Black: InfiniBand cables or AC power jumper cables

- Red: Integrated Lights Out Management (Oracle ILOM) Ethernet management cables

- Blue: Gigabit Ethernet management (eth0) cables

- Orange: KVM switch to dongle cables

## D.2 Oracle Big Data Appliance Rack Layout

Figure D-1 shows the front and rear layout of an Oracle Big Data Appliance rack.

Figure D-1 Rack Layout of Oracle Big Data Appliance

Description of "Figure D-1 Rack Layout of Oracle Big Data Appliance"

## D.3 KVM Network Cable Connections

A KVM switch is provided only in Sun Fire X4270 M2-based rack.

Table D-1 shows the keyboard, video, and mouse (KVM) network cabling to the servers. The cables are orange.

Table D-1 KVM Cabling

From Rack Unit | Component | To KVM Port
--- | --- | ---
U41 | Server 18 | 1
U39 | Server 17 | 2
U37 | Server 16 | 3
U35 | Server 15 | 4
U33 | Server 14 | 5
U31 | Server 13 | 6
U29 | Server 12 | 7
U28 | Server 11 | 8
U27 | Server 10 | 9
U26 | NM2-IB leaf switch | 10
U25 | KVM switch | 11
U19 | KVM tray | 12
U18 | Cisco switch | 13
U17 | NM2-IB leaf switch | 14
U16 | Server 9 | 15
U14 | Server 8 | 16
U12 | Server 7 | 17
U10 | Server 6 | 18
U8 | Server 5 | 19
U6 | Server 4 | 20
U4 | Server 3 | 21
U2 | Server 2 | 22

## D.4 Administrative Gigabit Ethernet Cable Connections

Table D-2 shows the cable connections for the administrative Gigabit Ethernet network (Net 0). The Ethernet switch is located in rack unit 21. The cables are 10 feet long and black.

Table D-2 Administrative Gigabit Ethernet Cabling

From Rack UnitFoot 1 | Component | To Ethernet Port
--- | --- | ---
U41 | Server 18 | 1
U39 | Server 17 | 3
U37 | Server 16 | 5
U35 | Server 15 | 7
U33 | Server 14 | 9
U31 | Server 13 | 11
U29 | Server 12 | 13
U27 | Server 11 | 17
U25 | Server 11 | 21
U24 | NM2-IB Switch | 45
U20 | NM2-IB Switch | 46
U18 | Server 10 | 25
U16 | Server 9 | 29
U14 | Server8 | 31
U12 | Server 7 | 33
U10 | Server 6 | 35
U8 | Server 5 | 37
U6 | Server 4 | 39
U4 | Server 3 | 41
U2 | NM2-IB Switch | 43
U1 | Server 2 | 47

Footnote 1 Un is the unit location in the rack, where n is the number.

## D.5 Oracle Integrated Lights Out Manager Cable Connections

Table D-3 shows the cable connections from the servers to the Oracle ILOM switch. The Oracle ILOM ports on the servers are labeled Net Mgt and connect to the Cisco Ethernet switch located in rack unit 21.

Table D-3 Oracle ILOM Cabling

From Rack UnitFoot 1 | Component | Ethernet Port | Cable Length | Cable Color
--- | --- | --- | --- | ---
U41 | Server 18 | 2 | 10 feet | Red
U39 | Server 17 | 4 | 10 feet | Red
U37 | Server 16 | 6 | 10 feet | Red
U35 | Server 15 | 8 | 10 feet | Red
U33 | Server 14 | 10 | 10 feet | Red
U31 | Server 13 | 12 | 10 feet | Red
U29 | Server 12 | 14 | 10 feet | Red
U27 | Server 11 | 18 | 10 feet | Red
U25 | Server 10 | 22 | 10 feet | Red
U18 | Server 9 | 26 | 10 feet | Red
U16 | Server 8 | 30 | 10 feet | Red
U14 | Server 7 | 32 | 10 feet | Red
U12 | Server 6 | 34 | 10 feet | Red
U10 | Server 5 | 36 | 10 feet | Red
U8 | Server 4 | 38 | 10 feet | Red
U6 | Server 3 | 40 | 10 feet | Red
U4 | Server 2 | 42 | 10 feet | Red
U2 | Server 1 | 44 | 10 feet | Red
PDU-A | PDU-A | 15 | 1 meter | White
PDU-B | PDU-B | 20 | 1 meter | White
Not applicable | Service | 48 | 10 feet | Blue

Footnote 1 Un is the unit location in the rack, where n is the number.

## D.6 Single-Phase Power Distribution Unit Cable Connections

Table D-4 shows the connections for single-phase cabling from each power distribution unit (PDU) to the power supplies in the rack. The cables terminate at PDU-A on the left and are routed to the right to enter the cable management arm (CMA). The cables are bundled in groups of four.

Table D-4 Single-Phase PDU Cabling

Rack UnitFoot 1 | PDU-A/PS-00 | PDU-B/PS-01 | Cable Length
--- | --- | --- | ---
U41 | G5-6 | G0-0 | 2 meters
U39 | G5-3 | G0-3 | 2 meters
U37 | G5-0 | G0-6 | 2 meters
U35 | G4-6 | G1-0 | 2 meters
U33 | G4-4 | G1-2 | 2 meters
U31 | G4-2 | G1-4 | 2 meters
U29 | G3-6 | G2-0 | 2 meters
U27 | G3-5 | G2-1 | 2 meters
U25 | G3-3 | G2-3 | 2 meters
U24 | G3-1 | G2-5 | 2 meters
U23 | Not Applicable | G3-0 | included
U22 | G2-5 | G3-1 | 1 meter
U21 | G3-0 | G2-6 | 2 meters
U20 | G2-4 | G3-2 | 2 meters
U18 | G2-2 | G3-4 | 2 meters
U16 | G1-6 | G4-0 | 2 meters
U14 | G2-0 | G3-6 | 2 meters
U12 | G1-4 | G4-2 | 2 meters
U10 | G1-2 | G4-4 | 2 meters
U8 | G1-0 | G4-6 | 2 meters
U6 | G0-6 | G5-0 | 2 meters
U4 | G0-4 | G5-2 | 2 meters
U2 | G0-2 | G5-4 | 2 meters
U1 | G0-0 | G5-6 | 2 meters

Footnote 1 Un is the unit location in the rack, where n is the number.

## D.7 Three-Phase Power Distribution Unit Cable Connections

Table D-5 describes three-phase cabling from each power distribution unit (PDU) to the power supplies in the rack. The cables are terminated to PDU-A on the left, are routed to the right to enter the cable management arm (CMA), and are bundled in groups of four.

Table D-5 Three-Phase PDU Cabling

Rack UnitFoot 1 | PDU-A/PS-00 | PDU-B/PS-01 | Cable Length
--- | --- | --- | ---
U41 | G5-6 | G2-0 | 2 meters
U39 | G5-3 | G2-3 | 2 meters
U37 | G5-0 | G2-6 | 2 meters
U35 | G4-6 | G1-0 | 2 meters
U33 | G4-4 | G1-2 | 2 meters
U31 | G4-2 | G1-4 | 2 meters
U29 | G3-6 | G0-0 | 2 meters
U27 | G3-5 | G0-1 | 2 meters
U25 | G3-3 | G0-3 | 2 meters
U24 | G3-1 | G0-5 | 2 meters
U23 | Not Applicable | G5-0 | Included
U22 | G2-5 | G5-1 | 1 meter
U21 | G3-0 | G0-6 | 2 meters
U20 | G2-4 | G5-2 | 2 meters
U18 | G2-2 | G5-4 | 2 meters
U16 | G1-6 | G4-0 | 2 meters
U14 | G2-0 | G5-6 | 2 meters
U12 | G1-4 | G4-2 | 2 meters
U10 | G1-2 | G4-4 | 2 meters
U8 | G1-0 | G4-6 | 2 meters
U6 | G0-6 | G3-0 | 2 meters
U4 | G0-4 | G3-2 | 2 meters
U2 | G0-2 | G3-4 | 2 meters
U1 | G0-0 | G3-6 | 2 meters

Footnote 1 Un is the unit location in the rack, where n is the number.

## D.8 In-Rack InfiniBand Switch-to-Switch Cable Connections

Table D-6 lists the location, ports, and cables for the InfiniBand connections from switch to switch. Figure D-2 identifies the locations of the ports on a Sun Network QDR InfiniBand Gateway switch.

Table D-6 InfiniBand Switch-to-Switch Cabling

From InfiniBand Switch Rack UnitFoot 1 | Port | To InfiniBand Switch Rack UnitFootref 1 | Port | Cable Length | Description
--- | --- | --- | --- | --- | ---
U20 | 9B | U24 | 9A | 2 meters | Leaf to leaf
U20 | 10B | U24 | 10A | 2 meters | Leaf to leaf
U20 | 11B | U24 | 11A | 2 meters | Leaf to leaf
U20 | 8A | U24 | 8A | 2 meters | Leaf to leaf
U20 | 9A | U24 | 9B | 2 meters | Leaf to leaf
U20 | 10A | U24 | 10B | 2 meters | Leaf to leaf
U20 | 11A | U24 | 11B | 2 meters | Leaf to leaf
U1 | 0B | U20 | 8B | 3 meters | Spine to leaf
U1 | 1B | U24 | 8B | 3 meters | Spine to leaf

Footnote 1 Un is the unit location in the rack, where n is the number.

Figure D-2 identifies the locations of the ports on a Sun Network QDR InfiniBand Gateway switch. Ports 5A, 5B, 6A, 6B, and 7A are available to connect to another device, such as Oracle Exalytics In-Memory Machine. Oracle recommends that you start with port 5A. Port 7B is reserved for future use by Oracle Big Data Appliance.

Figure D-2 Sun Network QDR InfiniBand Gateway Switch Ports

Description of "Figure D-2 Sun Network QDR InfiniBand Gateway Switch Ports"

## D.9 In-Rack InfiniBand Switch-to-Server Cable Connections

Table D-7 lists the location, ports, and cables for the InfiniBand connections from the leaf switches to the servers.

Table D-7 InfiniBand Switch-to-Server Cabling

From InfiniBand Switch Rack UnitFoot 1 | Port | To Rack UnitFootref 1 | PortFoot 2 | Cable Length
--- | --- | --- | --- | ---
U24 | 0A | U41 | PCIe 3 P1 | 3 meters
U24 | 0B | U39 | PCIe 3 P1 | 3 meters
U24 | 1A | U37 | PCIe 3 P1 | 3 meters
U24 | 1B | U35 | PCIe 3 P1 | 3 meters
U24 | 2A | U33 | PCIe 3 P1 | 3 meters
U24 | 2B | U31 | PCIe 3 P1 | 3 meters
U24 | 3A | U29 | PCIe 3 P1 | 3 meters
U24 | 3B | U27 | PCIe 3 P1 | 2 meters
U24 | 4A | U25 | PCIe 3 P1 | 2 meters
U20 | 0A | U41 | PCIe 3 P2 | 3 meters
U20 | 0B | U39 | PCIe 3 P2 | 3 meters
U20 | 1A | U37 | PCIe 3 P2 | 3 meters
U20 | 1B | U35 | PCIe 3 P2 | 3 meters
U20 | 2A | U33 | PCIe 3 P2 | 3 meters
U20 | 2B | U31 | PCIe 3 P2 | 3 meters
U20 | 3A | U29 | PCIe 3 P2 | 3 meters
U20 | 3B | U27 | PCIe 3 P2 | 2 meters
U20 | 4A | U25 | PCIe 3 P2 | 2 meters
U20 | 4B | U18 | PCIe 3 P1 | 2 meters
U20 | 12A | U16 | PCIe 3 P1 | 2 meters
U20 | 12B | U14 | PCIe 3 P1 | 3 meters
U20 | 13A | U12 | PCIe 3 P1 | 3 meters
U20 | 13B | U10 | PCIe 3 P1 | 3 meters
U20 | 14A | U8 | PCIe 3 P1 | 3 meters
U20 | 14B | U6 | PCIe 3 P1 | 3 meters
U20 | 15A | U4 | PCIe 3 P1 | 3 meters
U20 | 15B | U2 | PCIe 3 P1 | 3 meters
U24 | 4B | U18 | PCIe 3 P2 | 2 meters
U24 | 12A | U16 | PCIe 3 P2 | 2 meters
U24 | 12B | U14 | PCIe 3 P2 | 3 meters
U24 | 13A | U12 | PCIe 3 P2 | 3 meters
U24 | 13B | U10 | PCIe 3 P2 | 3 meters
U24 | 14A | U8 | PCIe 3 P2 | 3 meters
U24 | 14B | U6 | PCIe 3 P2 | 3 meters
U24 | 15A | U4 | PCIe 3 P2 | 3 meters
U24 | 15B | U2 | PCIe 3 P2 | 3 meters

Footnote 1 Un is the unit location in the rack, where n is the number.

Footnote 2 Pn is the InfiniBand port, where n is the port number.