Go to main content
27/32

# B Replacement Units

This appendix lists the replacement units for the components in Oracle Big Data Appliance racks. All replacement units are field replaceable units (FRUs), which are installed by Oracle field engineers.

This appendix contains the following sections:

- Understanding Repair Categories

- Disk Controller Batteries

- LED Status Descriptions

- Parts for Oracle Big Data Appliance Servers

- Parts for Sun Datacenter InfiniBand Switch 36

- Parts for Sun Network QDR InfiniBand Gateway Switch

- Parts for the Cisco Ethernet Switch

- Parts for Power Distribution Units

- Cables and Cable Accessories for an Oracle Big Data Appliance Rack

See Also:

"Spare Parts Kit Components"

## B.1 Understanding Repair Categories

Repair categories describe the potential effects of a repair action. Table B-1 describes the categories and related actions.

Table B-1 Oracle Big Data Appliance Repair Categories

Category | Description | Scenario Examples
--- | --- | ---
Hot Swap (HS) | The repair part is hot swappable and can be replaced without shutting down the host system. Procedures may be needed before and after replacement to protect the data. | Disks Fans Power supplies
Infrastructure Repair (IR) | Repair of a connectivity component within an Oracle Big Data Appliance rack. No downtime of the rack is required; however, individual components may require downtime. | External cables InfiniBand switch Ethernet switch
BDA Server Offline (BDA-O) | Repair of the part requires shutting down one Big Data Appliance server. No downtime of the rack is required; however, individual servers may require downtime and temporary removal from the cluster. Rebalancing the workload and data duplication may temporarily affect performance. If the system is currently running, then shut it down gracefully. See "Powering On and Off Oracle Big Data Appliance" for additional information. If you monitor the system using Oracle Enterprise Manager Cloud Control, then prevent unnecessary alerts by putting the target in a blackout state. Refer to Oracle Enterprise Manager Administration for additional information. | System boards PCIe cards Memory Processors

## B.2 Disk Controller Batteries

The disk controllers in the servers have battery-backed write cache to accelerate write performance. If the battery charge capacity degrades such that the battery cannot protect the cached data for a power loss of 48 hours or more, then the write cache is disabled and the disk controller switches to write through mode. This results in reduced write performance but no data loss. The servers generate an alert when the battery charge is insufficient, when the temperature is high, and when the battery should be replaced.

Battery charge capacity degrades over time, and the life expectancy of a battery is inversely proportional to the operating temperature. The worst-case life expectancy of a battery in an Oracle Big Data Appliance rack is as follows:

Inlet Ambient Temperature | Battery Lifetime
--- | ---
< 25 degrees Celsius (77 degrees Fahrenheit) | 3 years
< 32 degrees Celsius (90 degrees Fahrenheit) | 2 years

Oracle replaces failed batteries at no extra charge if the battery charge capacity in the disk controllers falls below the minimum threshold. As part of Oracle Premier Support for Systems, Oracle attempts to proactively replace the batteries in an Oracle Big Data Appliance rack before the end of the estimated lifetime, on a best effort basis.

## B.3 LED Status Descriptions

This section describes the light-emitting diodes (LEDs) in an Oracle Big Data Appliance rack. It contains these topics:

- Sun Server LEDs

- Sun InfiniBand Switch LEDs

### B.3.1 Sun Server LEDs

Table B-2 identifies some LED status indicators on the Sun Server X4-2L and X3-2L that can indicate a fault.

See Also:

"About Server and Component Status Indicators" in the Sun Server X4-2 Service Manual at

`http://docs.oracle.com/cd/E36975_01/html/E38045/z4000be71405942.html#scrolltoc`

Table B-2 Sun Server LED Status Descriptions

Component | LED Status
--- | ---
General Status | The following LEDs are located on the front and back panels of each server: Service Required (amber) Off indicates normal operation. Steady on indicates a fault in the server. Power/OK (green) Steady on indicates that the server is powered on. A slow blink indicates that the server is starting up. A steady blink indicates that standby power is on, but chassis power is off. Off indicates no AC power or an incomplete startup of Oracle ILOM.
Fans | Each fan module has one bicolored LED, which you can see when the top cover fan door is open. Fan Status (amber/green) Amber indicates that the fan module is faulty. The front and rear panel Service Required LEDs are also lit when the system detects a fan module fault. Green indicates that the system is powered on, and the fan module is functioning correctly.
Drives | The following LEDs are located on the storage and boot drives: Service Required (amber) Off indicates normal operation. Steady on indicates a fault in the drive. OK/Activity (green) Steady on indicates normal inactivity. A steady blink indicates normal activity. Off indicates that the power is off, or the system does not recognize the drive.
Power supply | The following LEDs are on each power supply. You can see them from the back of the server. Service Required (amber) Off indicates normal operation. Steady on indicates that the system has detected a problem in the power supply regarding the voltage, current, temperature, or fans. AC OK/DC OK (green) Steady on indicates normal operation for both AC and DC power. A slow blink indicates that input AC power is normal and output DC power is disabled. Off indicates no input AC power.

### B.3.2 Sun InfiniBand Switch LEDs

Table B-3 identifies some LED status indicators on Sun Datacenter InfiniBand Switch 36 and Sun Network QDR InfiniBand Gateway switches that can indicate a fault.

See Also:

- "Identifying LEDs" in the Sun Datacenter InfiniBand Switch 36 Service Manual at

  `http://docs.oracle.com/cd/E26698_01/html/E26434/z40000fe1394411.html`

- "Identifying LEDs" in the Sun Network QDR InfiniBand Gateway Switch Service Manual at

  `http://docs.oracle.com/cd/E26699_01/html/E26706/z40000fe1394411.html`

Table B-3 Sun InfiniBand Switch LED Status Descriptions

Component | LED Status
--- | ---
Chassis | The following LEDs are located on the left side of the rear panel. Attention (amber) Steady on indicates a fault. Off indicates normal operation. Flashing indicates no function. OK (green) Steady on indicates normal operation. Off indicates that the switch is off or initializing. Flashing indicates no function.
Link status | The link status LEDs are located by the data cable connectors on the rear panel. Link (green) Steady on indicates that a link is established. Off indicates that the link is down. Flashing indicates that there are symbol errors.
Network management ports | The following LEDs are located on the network management connector on the rear panel. Link Speed (amber/green): Green steady on indicates a 1000BASE-T link. Amber steady on indicates a 100BASE-T link. Off indicates no link. Flashing indicates no function. Activity (green): Flashing indicates packet activity. On indicates no function. Off indicates no activity.
Power supply | The following LEDs are located on the power supply at the front of the chassis. Attention (amber) Steady on indicates a fault, and 12 VDC is shut down. Off indicates normal operation. Flashing indicates no function. OK (green) Steady on indicates 12 VDC. Off indicates no DC voltage. Flashing indicates no function. AC LED is green Steady on indicates AC power is supplied. Off indicates that AC power is not present. Flashing indicates no function.
Fan | The following LED is located on the air inlet on the front of the chassis. FT On indicates a problem with the fan. Off indicates normal operation

## B.4 Parts for Oracle Big Data Appliance Servers

The following topics identify the replacement parts for the Oracle Big Data Appliance storage servers:

- Oracle Server X6-2L and X5-2L Parts

- Sun Server X4-2L Parts

- Sun Server X3-2L Parts

- Sun Fire X4270 M2 Parts

Note:

Oracle Big Data Appliance ships with two spare drives. If a drive is faulty, then the customer can replace the drive before an Oracle service representative arrives if circumstances warrant immediate action.

### B.4.1 Oracle Server X6-2L and X5-2L Parts

Figure B-1 shows the front view of the Oracle Server X6-2L and X5-2L. The hard drives are numbered from left to right, starting in the lower left. The drives in the bottom row are numbers 0, 1, 2, and 3. The drives in the middle row are numbers 4, 5, 6, and 7. The drives in the top row are numbers 8, 9, 10, and 11.

Figure B-1 Front View of Oracle Servers X6-2L and X5-2L

Description of "Figure B-1 Front View of Oracle Servers X6-2L and X5-2L"

Figure B-2 shows the rear view of a Oracle Server X6-2L or X5-2L storage server.

Figure B-2 Rear View of Oracle Servers X6-2L and X5-2L

Description of "Figure B-2 Rear View of Oracle Servers X6-2L and X5-2L"

Table B-4 lists the replaceable parts for the Oracle Server X6-2L and X5-2L, which are covered under the Oracle Premier Support for Systems warranty. The parts list for X6-2L and X5-2L are nearly the same except for CPUs and DIMMs. Unless otherwise noted, the repair procedures are in the Oracle Server X5-2L Service Manual.

Note:

All replacement parts listed in the following table are FRUs when covered under Premier Support of Systems warranty.

Table B-4 Replacement Parts for Oracle Server X6-2L and X5-2L Storage Servers

Part Number | Description | Repair Category | Repair Procedure
--- | --- | --- | ---
350-1719 | Assembly, 1U-2U Snap-in, slim rail rack | EBO | If the server is currently running, then shut it down gracefully. See "Powering On and Off Oracle Big Data Appliance". See "Reinstall the Server in the Rack" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.z40004191003899.html`
370-5621 | 3V lithium battery | EBO | See "Servicing the Battery" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.z40000f91037456.html`
7014226 | Cable, interlock, 125 mm | EBO | See "Servicing SAS Cables" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.baecfjbc.html`
7017231 | Indicator assembly, right | EBO | See "Servicing the Front LED/USB Indicator Modules" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.z40001d31014236.html`
7023515 | Disk backplane assembly, 2 rear | EBO | See "Servicing the Front and Rear Storage Drive Backplanes" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.z40007ac1419009.html`
7044130 | Power Supply, A258, 1000W, AC Input | HS | Remove rear left side of the CMA, and then swing it back and out to the right. The telescopic cross member supporting the cables directly behind the server can be retracted to access both power supplies. See "Servicing Power Supplies" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.z40000091014153.html` Replace the CMA.
7045042 | Fan assembly, 2U, 80 x 80, Ferrite, center rotate | HS | See "Servicing Fan Modules" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.z40000091014194.html`
3. 7046442 | Assembly, dual port, QDR CX3, host channel adapter | EBO | If the server is currently running, then shut it down gracefully. See "Powering On and Off Oracle Big Data Appliance". See "Servicing PCIe Cards" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.z40000f91037409.html` Verify that the new hardware meets the hardware and firmware specifications:
       # bdacheckhw
7064884 | Heat sink, CPU (Oracle Server X5-2L) | EBO | See "Servicing Storage Drives (CRU)" in Sun Server X5-2 Service Manual at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.z40001d31037480.html`
7067728 | Pre-Greased 1U CPU Heatsink (Oracle Server X6-2L) |  | See "Servicing Storage Drives (CRU)" in Sun Server X5-2 Service Manual at
7066824 | Assembly, drive, 8 TB, 3.5 inch, SAS/7200rpm | HS | See "Servicing Storage Drives and Rear Drives" in Sun Server X5-2 Service Manual at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.z40000091011460.html`
7069337 | Assembly, backplane, 12X3.5, W/SAS expansion, 2U | EBO | See "Servicing the Front and Rear Storage Drive Backplanes" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.z40007ac1419009.html`
7078071 | DIMM 16 GB (Oracle Server X5-2L) | EBO | See "Servicing the DIMMs" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.ceicjagi.html`
7310210 | 32GB DDR4-2400 DIMM (Oracle Server X6-2L) |  | See “Servicing the DIMMs” at `http://docs.oracle.com/cd/E62172_01/html/E62184/ceicjagi.html#scrolltoc`
7085209 | HBA, 12 Gb SAS PCIe 8-port RAID internal with flash module | EBO | See "Servicing the Oracle Storage 12 Gb/s SAS PCIe RAID HBA Card" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.gocfy.html`
7086345 | Assembly, super cap, 13.5 volt, 6.4F, SAS3 HBA | EBO | See "Servicing the Oracle Storage 12 Gb/s SAS PCIe RAID HBA Card" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.gocfy.html`
7086346 | Cable, super cap, 620M, 6-pin, straight, SAS3 HBA | EBO | See "Servicing SAS Cables" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.baecfjbc.html`
7090170 | Flash drive, MLC, OSA ID, USB, 8 GB | EBO | See "Servicing the Internal USB Flash Drives" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.ceiicfbd.html`
7095106 | CPU, 2.3GHz 18-Core E5-2699 (Oracle Server X5-2L) | EBO | Caution: Processors should be removed and replaced only by authorized Oracle Service personnel. `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.z40001d31037480.html`
7313670 | CPU, 22-Core 2.2GHz Intel E5-2699 v4, 145W (Oracle Server X6–2L) |  | Caution: Processors should be removed and replaced only by authorized Oracle Service personnel. `http://docs.oracle.com/cd/E62172_01/html/E62184/z40001d31037480.html#scrolltoc`
7096185 | Assembly, indicator, left | EBO | See "Servicing the Front LED/USB Indicator Modules" at `http://docs.oracle.com/cd/E41033_01/html/E48325/cnpsm.z40001d31014236.html`
7098504 | ASM, MOBO tray | EBO |

### B.4.2 Sun Server X4-2L Parts

Table B-6 lists the replaceable parts for the Sun Server X4-2L, which are covered under the Oracle Premier Support for Systems warranty. Unless otherwise noted, the repair procedures are in the Sun Server X4-2 Service Manual.

Table B-5 Replacement Parts for a Sun Server X4-2L Server

Part Number | Description | Repair Category | Repair Procedure
--- | --- | --- | ---
150-3993 | Battery, 3V, 390 MAH, LITH, COIN | BDA-O | See "Servicing the Battery" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40000f91037456.html#scrolltoc`
7090170 | 8 GB USB flash drive | BDA-O | See "Servicing the Internal USB Flash Drives" at `http://docs.oracle.com/cd/E36974_01/html/E38145/ceiicfbd.html#scrolltoc`
371-4985 | 6 Gigabit SAS RAID PCI battery module, RoHS:Y (LION), BBU-08 | BDA-O | Power down the server gracefully. See "Powering Off the Server for Orderly Shutdown" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40002401396307.html#scrolltoc` See Sun Storage 6 Gb SAS PCIe HBA, Internal Installation Guide For HBA Models SGX-SAS6-INT-Z and SG-SAS6-INT-Z (internal only) at `http://docs.oracle.com/cd/E19337-01/index.html`
7047503 | Niwot card | BDA-O | Power down the server gracefully. See "Powering Off the Server for Orderly Shutdown" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40002401396307.html#scrolltoc` See "Servicing PCIe Cards" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40000f91037409.html#scrolltoc`
7057184 | Assembly Battery Carrier Remote | HS | Oracle internal service documentation
7082397 | InfiniBand dual port, QDR CX3, HCA | BDA-O | Power down the server gracefully. See "Powering Off the Server for Orderly Shutdown" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40002401396307.html#scrolltoc` See "Servicing PCIe Cards" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40000f91037409.html#scrolltoc`
375-3701 | 6 Gbps SAS RAID disk PCIe HBA, RoHS:Y | BDA-O | Power down the server gracefully. See "Powering Off the Server for Orderly Shutdown" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40002401396307.html#scrolltoc` See "Servicing PCIe Cards" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40000f91037409.html#scrolltoc` Note: Do not run any controller commands when replacing the disk.
7066826 | Drive, 8 TB, 3.5", SAS/7200 RPM, CORAL | HS | See "Servicing Storage Drives" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40000091011460.html#scrolltoc` Do not run any controller commands when replacing the disk.
7014391 | SAS expander assembly | BDA-O | See "Servicing the SAS Expander Module" at `http://docs.oracle.com/cd/E36974_01/html/E38145/ceieidja.html#scrolltoc`
7020486 | DIMM, 8 GB, DDR3, 1600 MHz, 1.3V | BDA-O | See "Servicing the DIMMs" at `http://docs.oracle.com/cd/E36974_01/html/E38145/ceicjagi.html#scrolltoc`
7018704 | DIMM, 16 GB, DDR3, 1600 MHz, 1.35V | BDA-O | See "Servicing the DIMMs" at `http://docs.oracle.com/cd/E36974_01/html/E38145/ceicjagi.html#scrolltoc`
7041013 | DIMM, 32 GB, DDR3, RDIMM-1066, QUAD-RANK | BDA-O | See "Servicing the DIMMs" at `http://docs.oracle.com/cd/E36974_01/html/E38145/ceicjagi.html#scrolltoc`
7020774 | Pregreased CPU heatsink | BDA-O | See "Servicing Processors" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40001d31037480.html#scrolltoc`
7075289 | CPU, Intel E5-2650 v2 8-core 2.6 GHz | BDA-O | See "Servicing Processors" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40001d31037480.html#scrolltoc`
7044130 | Power supply, AC, A258, F, 12V, 1000W | HS | See "Servicing Power Supplies" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40000091014153.html#scrolltoc`
7045042 | Dual counter rotating fan module, 80x80 mm | HS | See "Servicing Fan Modules" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40000091014194.html#scrolltoc`
7047257 | 12-slot backplane cable kit with the following: Disk drive flex cable Dual backplane power cable Single backplane power cable Disk data cable, iPass+ HD to iPass+ HD, 600 mm | BDA-O | Shut down the rack. See "Powering On and Off Oracle Big Data Appliance". See "Servicing the Front and Rear Storage Drive Backplanes" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40007ac1419009.html#scrolltoc`
7047768 | 12-slot 3.5" disk cage, including fan door, and left and right ear assembly | BDA-O | Shut down the rack. See "Powering On and Off Oracle Big Data Appliance". See "Servicing the Front and Rear Storage Drive Backplanes" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40007ac1419009.html#scrolltoc`
7049382 | System board assembly, RoHS:Y | BDA-O | Shut down the rack. See "Powering On and Off Oracle Big Data Appliance". "Servicing the Motherboard Assembly" at `http://docs.oracle.com/cd/E36974_01/html/E38145/z40001d31037512.html#scrolltoc`

### B.4.3 Sun Server X3-2L Parts

Table B-6 lists the replaceable parts for the Sun Server X3-2L, which are covered under the Oracle Premier Support for Systems warranty. Unless otherwise noted, the repair procedures are in the Sun Server X3-2L Service Manual.

Table B-6 Replacement Parts for a Sun Server X3-2L Server

Part Number | Description | Repair Category | Repair Procedure
--- | --- | --- | ---
150-3993 | Battery, 3V, 390 MAH, LITH, COIN | BDA-O | See "Servicing the Battery" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z40000f91037456.html#scrolltoc` Note: Rear storage drive 1 might be populated with a remote battery module for the host bus adapter (HBA) card. See "Remove a Rear Storage Drive" at `http://docs.oracle.com/cd/E23393_01/html/E27229/bbggjgea.html#scrolltoc`
7090170 | 8 GB USB flash drive | BDA-O | See "Servicing the Internal USB Flash Drives" at `http://docs.oracle.com/cd/E23393_01/html/E27229/ceiicfbd.html#scrolltoc`
371-4985 | 6 Gigabit SAS RAID PCI battery module, RoHS:Y (LION), BBU-08 | BDA-O | Power down the server gracefully. See "Powering Down the Server" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z400061b1011735.html` See Sun Storage 6 Gb SAS PCIe HBA, Internal Installation Guide For HBA Models SGX-SAS6-INT-Z and SG-SAS6-INT-Z (internal only) at `http://docs.oracle.com/cd/E19337-01/index.html`
7047503 | Niwot card | BDA-O | Power down the server gracefully. See "Powering Down the Server" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z400061b1011735.html` See "Servicing PCIe Cards" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z40000f91037409.html`
7057184 | Assembly Battery Carrier Remote | HS | See "Remove a Rear Storage Drive" at `http://docs.oracle.com/cd/E23393_01/html/E27229/bbggjgea.html#scrolltoc`
375-3696 | InfiniBand (CX2) dual port CX2 4x QDR PCI-e | BDA-O | Power down the server gracefully. See "Powering Down the Server" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z400061b1011735.html` See "Servicing PCIe Cards" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z40000f91037409.html`
375-3701 | 6 Gbps SAS RAID disk PCIe HBA, RoHS:Y | BDA-O | Power down the server gracefully. See "Powering Down the Server" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z400061b1011735.html` See "Servicing PCIe Cards" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z40000f91037409.html` Note: Do not run any controller commands when replacing the disk.
7010036 | DR 3 TB, 3.5-inch, SAS/7200, CORAL | HS | See "Servicing Storage Drives and Rear Drives" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z40000091011460.html` Do not run any controller commands when replacing the disk. Note: Rear storage drive 1 might be populated with a remote battery module for the host bus adapter (HBA) card. See "Remove a Rear Storage Drive" at `http://docs.oracle.com/cd/E23393_01/html/E27229/bbggjgea.html#scrolltoc`
7014391 | SAS expander assembly | BDA-O | See "Servicing the SAS Expander Module" at `http://docs.oracle.com/cd/E23393_01/html/E27229/ceieidja.html`
7020486 | DIMM, 8 GB, DDR3, 1600 MHz, 1.3V | BDA-O | See "Servicing the DIMMs" at `http://docs.oracle.com/cd/E23393_01/html/E27229/ceicjagi.html#scrolltoc`
7018704 | DIMM, 16 GB, DDR3, 1600 MHz, 1.35V | BDA-O | See "Servicing the DIMMs" at `http://docs.oracle.com/cd/E23393_01/html/E27229/ceicjagi.html#scrolltoc`
7041013 | DIMM, 32 GB, DDR3, RDIMM-1066, QUAD-RANK | BDA-O | See "Servicing the DIMMs" at `http://docs.oracle.com/cd/E23393_01/html/E27229/ceicjagi.html#scrolltoc`
7020774 | Pregreased CPU heatsink | BDA-O | See "Servicing Processors" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z40001d31037480.html#scrolltoc`
7026881 | CPU,Intel,E5-2660,2.2 GHz, 8-core | BDA-O | See "Servicing Processors" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z40001d31037480.html#scrolltoc`
7044130 | Power supply, AC, A258, F, 12V, 1000W | HS | See "Servicing Power Supplies" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z40000091014153.html`
7045042 | Dual counter rotating fan module, 80x80 mm | HS | See "Servicing Fan Modules" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z40000091014194.html`
7047257 | 12-slot backplane cable kit with the following: Disk drive flex cable Dual backplane power cable Single backplane power cable Disk data cable, iPass+ HD to iPass+ HD, 600 mm | BDA-O | Shut down the rack. See "Powering On and Off Oracle Big Data Appliance". See "Servicing the Front and Rear Storage Drive Backplanes" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z40007ac1419009.html`
7047768 | 12-slot 3.5" disk cage, including fan door, and left and right ear assembly | BDA-O | Shut down the rack. See "Powering On and Off Oracle Big Data Appliance". See "Servicing the Front and Rear Storage Drive Backplanes" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z40007ac1419009.html`
7049382 | System board assembly, RoHS:Y | BDA-O | Shut down the rack. See "Powering On and Off Oracle Big Data Appliance". "Servicing the Motherboard Assembly" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z40001d31037512.html`

### B.4.4 Sun Fire X4270 M2 Parts

Table B-7 lists the replaceable parts for the Sun Fire X4270 M2, which are covered under the Oracle Premier Support for Systems warranty. Unless otherwise noted, the repair procedures are in the Sun Fire X4270 M2 Server Service Manual.

Table B-7 Replacement Parts for Sun Fire X4270 M2 Servers

Part Number | Description | Repair Category | Repair Procedure
--- | --- | --- | ---
150-3993 | Battery, 3V, 390 MAH, LITH, COIN | BDA-O | See Section 4.6, "Servicing the Server Battery" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/motherboard.html#50438179_71528`
300-2235 | Power supply, A249, 1200W, 12V, 2U, RoHS:Y | HS | See Section 3.4, "Servicing Power Supplies" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/hotswap.html#50438178_11706`
350-1502 | Universal rack mount kit | BDA-O | If the system is currently running, then shut it down gracefully. See "Powering On and Off Oracle Big Data Appliance." See Chapter 2, "Installing the Server Into a Rack With Slide-Rails" in Sun Fire X4170 M2 and X4270 M2 Servers Installation Guide at `http://docs.oracle.com/cd/E19245-01/E27205/z4000c671007752.html`
7090170 | 8 GB USB flash drive | BDA-O | Not applicable
371-4966 | LV DIMM, 8 GB, DDR3, 1RX4, 1333 MHz | BDA-O | See Section 4.2, "Servicing Memory Modules (DIMMs)" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/motherboard.html#50438179_71526`
371-4982 | 6 Gigabit SAS RAID PCI battery module, RoHS:Y (LION), BBU-08 | BDA-O | If the system is currently running, then shut it down gracefully. See "Powering On and Off Oracle Big Data Appliance." See Sun Storage 6 Gb SAS PCIe HBA, Internal Installation Guide For HBA Models SGX-SAS6-INT-Z and SG-SAS6-INT-Z (internal only) at `http://docs.oracle.com/cd/E19337-01/index.html`
375-3696 | InfiniBand (CX2) dual port CX2 4x QDR PCI-e | BDA-O | If the system is currently running, then shut it down gracefully. See "Powering On and Off Oracle Big Data Appliance." See Section 4.5, "Servicing PCIe Cards" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/motherboard.html#50438179_86021`
375-3701 | 6 Gbps SAS RAID disk PCIe HBA, RoHS:Y | BDA-O | If the system is currently running, then shut it down gracefully. See "Powering On and Off Oracle Big Data Appliance." See Section 4.5, "Servicing PCIe Cards" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/motherboard.html#50438179_86021` Note: Do not run any controller commands in the service manual when replacing the disk.
530-3927 | Cable, PDB, MB, 1U+2U, ribbon | BDA-O | See Section 5.10, "Servicing Cables " in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/infrastructure_x4270_M2.html#50438167_58217`
530-4228 | Cable, mini-SAS, 36 POS LONG, LY, RoHS:Y | BDA-O | See Section 5.10, "Servicing Cables" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/infrastructure_x4270_M2.html#50438167_78806`
541-2075 | Bus_bar, power, 1U+2U, RoHS:Y | BDA-O | See Section 5.6, "Servicing the Power Distribution Board" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/infrastructure_x4270_M2.html#50438167_85936`
541-2884 | Assembly, riser, X8, X8, 2U, PCI-E, RoHS:Y | BDA-O | See Section 4.4, "Servicing PCIe Risers" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/motherboard.html#50438179_53252`
541-3310 | Xeon Heatsink with grease, RoHS:Y, 2U | BDA-O | See Section 4.7, "Servicing CPUs" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/motherboard.html#50438179_23425`
541-3356 | x8/x8 switched PCIe riser assembly, RoHS:Y with the following: x8/x8 switch PCIe riser bracket | BDA-O | If the system is currently running, then shut it down gracefully. See "Powering On and Off Oracle Big Data Appliance." See Section 4.4, "Servicing PCIe Risers" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/motherboard.html#50438179_53252`
541-4081 | System board assembly, RoHS:Y | BDA-O | If the system is currently running, then shut it down gracefully. See "Powering On and Off Oracle Big Data Appliance." See Section 4.8, "Servicing the Motherboard" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/motherboard.html#50438179_98526`
541-4124 | Fan deck, Hyde, RoHS:Y | BDA-O | See Section 5.3, "Servicing the Fan Board" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/infrastructure_x4270_M2.html#50438167_71556`
541-4222 | Assembly, fan, CR, 2U, RoHS:Y | HS | See Section 3.3, "Servicing Fan Modules" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/hotswap.html#50438178_28930`
541-4223 | Power distribution board, 2U, RoHS:Y | BDA-O | See Section 5.6, "Servicing the Power Distribution Board" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/infrastructure_x4270_M2.html#50438167_71558`
541-4304 | Indicator, right, Hyde 12/24, RoHS:Y | BDA-O | See Section 5.5, "Servicing the Front Panel LED Modules" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/infrastructure_x4270_M2.html#50438167_71563`
541-4305 | Assembly, disk, SAS2, XP_DC, Hyde, RoHS:Y | BDA-O | See Section 5.2, "Servicing the SAS Expander Board" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/infrastructure_x4270_M2.html#50438167_28246`
541-4306 | Assembly, connector board bracket, Hyde | BDA-O | See Section 5.7, "Servicing the Connector Board" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/infrastructure_x4270_M2.html#50438167_pgfId-1296581`
541-4363 | 12-slot disk backplane, RoHS:Y | BDA-O | See Section 5.4, "Servicing the Disk Backplane" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/infrastructure_x4270_M2.html#50438167_71557`
541-4371 | Indicator, left, Hyde 12/24, RoHS:Y | BDA-O | See Section 5.5, "Servicing the Front Panel LED Modules" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/infrastructure_x4270_M2.html#50438167_71563`
560-2952 | Cable kit, Hyde, RoHS:Y with the following: Disk backplane power cable 24-slot DBP power cable 12/24 slot disk backplane signal cable Fan signal cable Fan power cable | BDA-O | Refer to the entries for the individual items in the kit.
7010036 | FRU DR 3 TB 3.5-inch SAS/7200, CORAL | -- | See Section 3.2, "Servicing Storage Drives and Boot Drives" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/hotswap.html#50438178_61628` Note: Do not run any controller commands in the service manual when replacing the disk.
7012433 | 3.06 GHz processor | BDA-O | See Section 4.7, "Servicing CPUs" in Sun Fire X4270 M2 Server Service Manual at `http://docs.oracle.com/cd/E19245-01/821-0488-12/motherboard.html#50438179_23425`

## B.5 Parts for Sun Datacenter InfiniBand Switch 36

Table B-8 lists the replaceable parts for the Sun Datacenter InfiniBand Switch 36, which are covered under the Oracle Premier Support for Systems warranty. Unless otherwise noted, the repair procedures reference the Sun Datacenter InfiniBand Switch 36 Service Manual at

`http://docs.oracle.com/cd/E26698_01/index.html`

See "Cables and Cable Accessories for an Oracle Big Data Appliance Rack" for information about InfiniBand cables.

Table B-8 Replacement Parts for the Sun Datacenter InfiniBand Switch 36

Part Number | Description | Repair Category | Repair Procedure
--- | --- | --- | ---
7081595 | A247A, 12V, 760-watt power supply, RoHS:Y | HS | See "Servicing Power Supplies" at `http://docs.oracle.com/cd/E26698_01/html/E26434/z40001f49112.html`
350-1312 | Fan module for Sun Datacenter InfiniBand Switch 36, RoHS:Y | HS | See "Servicing Fans" at `http://docs.oracle.com/cd/E26698_01/html/E26434/z40001f59112.html`
371-2210 | CR2032 3V battery, RoHS:Y | IR | See "Servicing the Battery" at `http://docs.oracle.com/cd/E26698_01/html/E26434/z40001f79112.html`
541-3495 | Sun Datacenter InfiniBand Switch 36, RoHS:YL | IR | See "Replacing a Failed InfiniBand Switch". See "Installing the Switch" in the Sun Datacenter InfiniBand Switch 36 Installation Guide at `http://docs.oracle.com/cd/E26698_01/html/E26434/cggfbhhf.html`
594-6603 | 10 Gbps QSFP short wavelength transceiver | IR | See "Servicing Data Cables" at `http://docs.oracle.com/cd/E26698_01/html/E26434/z40001f69112.html`

## B.6 Parts for Sun Network QDR InfiniBand Gateway Switch

Table B-9 lists the replaceable parts for the Sun Network QDR InfiniBand Gateway switch, which are covered under the Oracle Premier Support for Systems warranty. Unless otherwise noted, the repair procedures refer to the Sun Network QDR InfiniBand Gateway Switch Service Manual at

`http://docs.oracle.com/cd/E26699_01/index.html`

See "Cables and Cable Accessories for an Oracle Big Data Appliance Rack" for information about InfiniBand cables.

Table B-9 Replacement Parts for the Sun Network QDR InfiniBand Gateway Switch

Part Number | Description | Repair Category | Repair Procedure
--- | --- | --- | ---
7081595 | A247A, 12V, 760-watt power supply, RoHS:Y | HS | See "Servicing Power Supplies" at `http://docs.oracle.com/cd/E26699_01/html/E26706/z40001f49112.html`
350-1312 | Fan module, RoHS:Y | HS | See "Servicing Fans" at `http://docs.oracle.com/cd/E26699_01/html/E26706/z40001f59112.html`
371-2210 | CR2032 3V battery, RoHS:Y | IR | See "Servicing the Battery" at `http://docs.oracle.com/cd/E26699_01/html/E26706/z40001f79112.html`
594-6603 | 10 Gbps QSFP short wavelength transceiver | IR | See "Servicing Data Cables" at `http://docs.oracle.com/cd/E26699_01/html/E26706/z40001f69112.html`
7014378 | Assembly, system, NM2-Gateway | IR | See "Replacing a Failed InfiniBand Switch". See "Installing the Gateway" in the Sun Network QDR InfiniBand Gateway Switch Installation Guide at `http://docs.oracle.com/cd/E26699_01/html/E26706/cggfbhhf.html`

## B.7 Parts for the Cisco Ethernet Switch

Table B-10 lists replaceable parts for the Cisco Ethernet switch, which are covered under the Oracle Premier Support for Systems warranty.

See Also:

Cisco Catalyst 4948E and Catalyst 4948E-F Switch Installation Guide at

`http://www.cisco.com/en/US/docs/switches/lan/catalyst4900/4948E/installation/guide/4948E_ins.html`

Table B-10 Replacement Parts for Cisco Catalyst Ethernet

Part Number | Description | Repair Category | Repair
--- | --- | --- | ---
7055121 | Cooling fan tray | HS | See Chapter 4 of the Cisco Catalyst 4948E and Catalyst 4948E-F Switch Installation Guide.
7055122 | Power supply, redundant | HS | See Chapter 4 of the Cisco Catalyst 4948E and Catalyst 4948E-F Switch Installation Guide.
7055123 | SNET, WS-C4948E-F | IR | See Chapter 3 of the Cisco Catalyst 4948E and Catalyst 4948E-F Switch Installation Guide.

## B.8 Parts for Power Distribution Units

Table B-11 lists the replacement parts for the power distribution units (PDUs), which are covered under the Oracle Premier Support for Systems warranty. The repair procedures references the Sun Rack II Power Distribution Units User's Guide at

`http://docs.oracle.com/cd/E19844-01/html/E29153/index.html`

Because of the number of cables and connections, Oracle recommends shutting down the Oracle Big Data Appliance rack during the replacement of power distribution unit parts.

Table B-11 Replacement Parts for Power Distribution Units

Part Number | Description | Repair Category | Repair Procedures
--- | --- | --- | ---
180-2379 | 13A/250V 90 degree IEC 320 Sheet E to IEC 320 C13 cord, 1 meter, RoHS:Y | HS | Not applicable
180-2380 | 13A/250V 90 degree IEC 320 Sheet E to IEC 320 C13 cord, 2 meter, RoHS:Y | HS | Not applicable
371-3995 | Three-phase PDU: 15 kVA, IEC309 60A, 4-pin, 250 VAC, three-phase IP67, North America, RoHS:Y | IR | See "Removing and Replacing PDUs" at `http://docs.oracle.com/cd/E19844-01/E23956/z40000121011643.html#scrolltoc`
371-4976 | Three-phase PDU: 15 kVA, 5-pin, IEC309 32A, 5-pin 230/400V, three-phase IP44, international, RoHS:Y | IR | See "Removing and Replacing PDUs" at `http://docs.oracle.com/cd/E19844-01/E23956/z40000121011643.html#scrolltoc`
371-4199 | Single-phase PDU: 15 kVA, with three 30A/250V 2-pole/3-wire NEMA L6-30P plugs, North America, RoHS:Y | IR | See "Removing and Replacing PDUs" at `http://docs.oracle.com/cd/E19844-01/E23956/z40000121011643.html#scrolltoc`
371-5040 | Single-phase PDU: 22 kVA, with three blue 32A/240V splash-proof 2-pole/3-wire IEC 60309 plugs, international, RoHS:Y | IR | See "Removing and Replacing PDUs" at `http://docs.oracle.com/cd/E19844-01/E23956/z40000121011643.html#scrolltoc`

## B.9 Cables and Cable Accessories for an Oracle Big Data Appliance Rack

Table B-12 lists the replacement cables and cable accessories for an Oracle Big Data Appliance rack, which are covered under the Oracle Premier Support for Systems warranty.

See Also:

- Sun Network QDR InfiniBand Gateway Switch Service Manual at

  `http://docs.oracle.com/cd/E26699_01/html/E26706/gentextid-26783.html#scrolltoc`

- Sun Datacenter InfiniBand Switch 36 Service Manual at

  `http://docs.oracle.com/cd/E26698_01/html/E26434/gentextid-21904.html#scrolltoc`

- See Cisco Catalyst 4948E and Catalyst 4948E-F Switch Installation Guide at

  `http://www.cisco.com/en/US/docs/switches/lan/catalyst4900/4948E/installation/guide/4948E_ins.html`

Table B-12 Replacement Cables for an Oracle Big Data Appliance Rack

Part Number | Description | Repair Category | Repair
--- | --- | --- | ---
350-1287 | Slim rail, CMA, 1U-2U for Sun servers | BDA-O | Power down the server gracefully. See "Powering Down the Server" at `http://docs.oracle.com/cd/E23393_01/html/E27229/z400061b1011735.html` See "Install Cable Management Arm" in the Sun Server X3-2L Installation Guide at `http://docs.oracle.com/cd/E23393_01/html/E27229/z40000401014951.html`
350-1519 | Serial cable kit, RoHS:Y with the following: USB to DB 9-pin M serial cable DB 9-pin F to DB 9-pin F null modem cable | HS | See "Understanding Cabling" in the Sun Datacenter InfiniBand Switch 36 Installation Guide at `http://docs.oracle.com/cd/E26698_01/html/E26434/cggfhjcc.html`
530-4567 | 4x QSFP copper QDR InfiniBand cable, 2 m, RoHS:Y | HS | See "Maintaining the InfiniBand Network". See "Understanding Cabling" in the Sun Datacenter InfiniBand Switch 36 Installation Guide at `http://docs.oracle.com/cd/E26698_01/html/E26434/cggfhjcc.html` Note: Redundancy is lost during cable replacement.
530-4445 | 4x QSFP copper QDR InfiniBand cable, 3 m, RoHS:Y | HS | See "Maintaining the InfiniBand Network". See "Understanding Cabling" in the Sun Datacenter InfiniBand Switch 36 Installation Guide at `http://docs.oracle.com/cd/E26698_01/html/E26434/cggfhjcc.html`
530-4446 | 4x QSFP copper QDR InfiniBand cable, 5 m, RoHS:Y | HS | See "Maintaining the InfiniBand Network". See "Understanding Cabling" in the Sun Datacenter InfiniBand Switch 36 Installation Guide at `http://docs.oracle.com/cd/E26698_01/html/E26434/cggfhjcc.html`
530-4432 | Ethernet cable, Cat 5/5E, RJ45 to RJ45, 7 foot, blue, RoHS:Y | HS | See Cisco Catalyst 4948E and Catalyst 4948E-F Switch Installation Guide.
530-4433 | Ethernet cable, Cat 5/5E, RJ45 to RJ45, 10 foot, red, RoHS:Y | HS | See Cisco Catalyst 4948E and Catalyst 4948E-F Switch Installation Guide.
530-4434 | Ethernet cable, Cat 5/5E, RJ45 to RJ45, 7 foot, red, RoHS:Y | HS | See Cisco Catalyst 4948E and Catalyst 4948E-F Switch Installation Guide.
530-4435 | Ethernet cable, Cat 5/5E, RJ45 to RJ45, 10 foot, black, RoHS:Y | HS | See Cisco Catalyst 4948E and Catalyst 4948E-F Switch Installation Guide.
530-4436 | Ethernet cable, Cat 5/5E, RJ45 to RJ45, 7 foot, black, RoHS:Y | HS | See Cisco Catalyst 4948E and Catalyst 4948E-F Switch Installation Guide.