         --------------------------------------------------------
                   TWAIN Data source Software
                        < 32-bit version >
                           README File
                           18, July. 2003
                         Version 9.11.32.0
         --------------------------------------------------------

                Copyright (C) PFU LIMITED 1995-2003


Please read this file before using this product.  The file includes 
important notes and also the latest additional information not included
in the on-line help.

------------------------------------------------------------------------
Table of Contents 
------------------------------------------------------------------------

1. System Requirement
2. How to install
3. Note on power management
4. When using the Adaptec-made SCSI adapter in IBM PC/AT Compatible machine
5. Notes on Two or more scanner devices at same PC.
6. Notes on duplex-scanning feature
7. Notes on scanning-area specification 
8. Notes on document-jam
9. Notes on 256 color and 8 color
10. Cautions on Automatic Size and Skew Detection
11. Notes on Automatic Page Size Detection
12. Notes on power-off during scanning
13. Notes on system font
14. Notes on SCSI BIOS setting
15. Notes on Job Contorol with Cache Mode
16. High Safety Required Use


-------------------------------------------------------------
1. System Requirement
-------------------------------------------------------------

This software is required following environments.

  1) CPU
     IBM PC/AT and/or compatible machine supported SCSI-2 or USB 1.1
     
  2) Operating System
     - Microsoft(R) Windows(R) 98
     - Microsoft(R) Windows(R) 98 Second
     - Microsoft(R) Windows(R) Me
     - Microsoft(R) Windows(R) 2000 Professional
     - Microsoft(R) Windows(R) XP Home Edition
     - Microsoft(R) Windows(R) XP Professional


-------------------------------------------------------------
2. How to install
-------------------------------------------------------------

 - In case of installer included by CD-ROM/CD-R media
   Follow the instruction on star-up dialog starting by inserting CD-ROM media.

 - In case of installer provided by Web or other media
   Run "setup.exe" and follow the instruction on the screen.

 - The user must log in with administrator authority.
   For information on logging in with the proper authority, contact the system 
   administrator.


---------------------------------------------------
3. Notes on power management 
---------------------------------------------------

If a PC turns to stand-by or suspend/resume when a scanner is scanning documents,
the next scanning does not usually perform collectly.
In this case, please reboot a scanner and scan again.


-------------------------------------------------------------
4. When using the Adaptec-made SCSI adapter 
   in IBM PC/AT Compatible machine
-------------------------------------------------------------

The TWAIN data source supports the below Adaptec-made SCSI adapter in the IBM 
PC/AT Compatible machine. 

 - SCSI Card 19160 (ASC-19160 for PCI bus)
 - SCSI Card 2910C (AHA-2910C for PCI bus)
 - SCSI Card 2940AU (AHA-2940AU for PCI bus)
 - PCI Ultra SCSI Master Kit (AHA-2940U for PCI bus)
 - SlimSCSI 1460 (APA-1460A/AHA-1460B for PCMCIA bus)

fi-4990C and fi-4860C were checked only on the following SCSI adapter.

 - Kofax Adrenaline 650i


---------------------------------------------------
5. Notes on Two or more scanner devices at same PC.
---------------------------------------------------

On Windows2000, this software does not support multi-device.
If two or more devices are connected to one PC, use version 8.10 of this 
software which using ASPI interface.

When using USB interface, this software does not support multi-device.


---------------------------------------------------
6. Notes on duplex-scanning feature
---------------------------------------------------

To use the duplex scanning feature in this software, the application you use 
must support the continuous-scanning feature of image data.

Thus, duplex-image data may not be scanned depending on the application, even 
though the duplex-scanning is specified. 


---------------------------------------------------
7. Notes on scanning-area specification
---------------------------------------------------

Scanning-area can be specified using the 3-type units such as millimeter(mm), 
inch, and pixel. However, please note, the scanning area may have an error of 
max.32-pixel per one line in each unit. 


---------------------------------------------------
8. Notes on paper-jam 
---------------------------------------------------

When paper-jam occurs, the error message: "Paper Jam" is displayed.
 
After the jammed documents was pulled out and the OK button on the error-message
 dialogue was pressed, the software becomes input-ready condition, and scanning 
is ready to be started. 

However, regarding the simplex scanning (duplex-scanning is not specified), in 
the case that paper-jam occurs while the top of the document is being scanned, 
one extra document may be ejected out of the documents on the tray when pressing
 the OK button in the error-message dialogue.
In this case, return the ejected document back to the tray and start to scan 
again.


---------------------------------------------------
9. Notes on 256 color and 8 color
---------------------------------------------------

This software supports 256 color and 8 color. We know that there are some 
software applications do not provide support for these two functions. They are 
Adobe Photo Shop and Adobe Acrobat which produce a all black image.
We recommend you to use Image Professional 2.6 or Imaging on Windows OS and 
ScandAll2001 V.4.0 (or greater) for these two color features. Or simply not use 
256 color and 8 color if you do not need to.


---------------------------------------------------
10. Cautions on Automatic Size and Skew Detection
---------------------------------------------------

This driver has a function to detect document size and skew automatically and provide 
corrected output. However, certain applications do not support this function and may 
not work properly, or the output image may get corrupted. The following applications 
were found to have the problems. If you use these applications, please disable 
[Automatic Size and Skew Detection] function. 
 - Adobe Photoshop
 - Adobe Acrobat 


---------------------------------------------------
11.Notes on Automatic Page Size Detection
---------------------------------------------------

When Halftone, SEE or Automatic Separation scan mode selected with Automatic 
Page Size Detection turned on,
It depends on whether white/black pixel and paper size detected the time while 
scanning. 
If the while pixel is detected, it usually produces correct image as expected.
Otherwise, it doesnot produce correct image which may has a black frame 
surrounded.
It is the nature of Halftone, SEE and Automatic Separation image which filled 
with Black/White pixels and is also the limitation of Automatic Page Size 
Detection function.


---------------------------------------------------
12. Notes on power-off during scanning
---------------------------------------------------

If power cable or interface cable of scanner is detached during scanning, this 
software may be terminated illeagally.
So, please do not remove them during the scanner is scanning.


---------------------------------------------------
13. Notes on System font
---------------------------------------------------

Some string on dialog box of this software is cut off, if the system-font is 
changed to LARGE or greater. It is depending on a using OS and graphic 
accelerator and display drivers.
depending on graphic accelerator and display driver that you use.  
In this case, select smaller system-font for the normal display.   


---------------------------------------------------
14.  Notes on SCSI BIOS setting
---------------------------------------------------

Also, when using the software, the setting for DISCONNECT on SCSI board must be 
valid.

When using the SCSI boards described in the above "4",  the changing is not 
required because the standard setting value is already set to "DISCONNECT 
Enable".
  
For the detailed setting-procedures, please refer to the instruction manual 
attached to the SCSI board that you use.   


---------------------------------------------------
15. Notes on Job Control with Cache Mode
---------------------------------------------------

With some scanner devices:fi-4860C, fi-4990C, and M4099D, "Use Both Memory" or 
"Use Memory on Scanner" appear in "Cache Mode" of the software's option dialog.
But, if "Use Both Memory" or "Use Memory on Scanner" is selected, "Job Control" 
setting is ignored in same option dialog.


---------------------------------------------------
16. High Safety Required Use
---------------------------------------------------

This Product is designed, developed and manufactured as contemplated for 
general use, including without limitation, general office use, personal use, 
household use, and ordinary industrial use, but is not designed, developed 
and manufactured as contemplated for use accompanying fatal risks or dangers 
that, unless extremely high safety is secured, could lead directly to death, 
personal injury, severe physical damage or other loss (hereinafter 
"High Safety Required Use"), including without limitation, nuclear power 
reactioncore control in nuclearatomic facility, airplane automaticaircraft 
flight control, air traffic control, operation control in mass transport 
controlsystem, medical instrument for life support system, missile launching 
control in weapon system. 
You shall not use this Product without securing the sufficient safety 
required for the High Safety Required Use. 
In addition, PFU (or other affiliated company) shall not be liable against 
the Customer and/or any third party for any claims or damages arising in 
connection with the High Safety Required Use of the Product.


------------------------------------------------------------------------
Microsoft, Windows and Windows NT are registered trademarks of Microsoft 
Corporation in the United States and/or other countries.
Other company name and product name are trademarks or registered trademarks of 
individual companies.
