  InSight

# Launching InSight

  InSight is launched from the Unit Detail window. To bring up Unit Detail, double-click on the unit you wish to monitor.
  DLCI has a listed reference in the table for each port of the FRAP. If a VNIP partner exists, VNIP delay will only be available if InSight is launched on the port connected to the partner. Since in most cases, FRAPs will be connected to their VNIP partner on the Network Port, users may wish to launch InSight from the Network Port, not the DTE Port.
  Once Unit Detail launches, select a DLCI, then click your right mouse button to access the pop-up menu. VNIP Partner information can be viewed.
  From the pop-up menu, select InSight.
  Note: If this option is grayed out, you do not have the InSight application installed.