  CONFIGURATION EDITOR
  FILTERING

# SNA/LLC2 Filtering

Filter Out SNA/LLC2 Frames

  Enable (select) this feature if you want to filter SNA/LLC2 frames on all routes.

Virtual-Port Specific Filtering Overrides

  This feature enables you to specify filtering overrides for certain ports and DLCIs. These filters will override the default filter setting
  1. Click on the Add button.
  2. Click inside the port field to select a port.
  3. Click inside the DLCI field and enter the provider-assigned DLCI number.
  4. Click inside the Filter Out SNA/LLC2 Frames field to set the filtering to Yes or No.
  Range: Ports: 1 --8, DLCIs: 16 -- 1023, Filter Frames: Yes or No
  Also See Bridge Filtering