# CONFIGURATION EDITOR

# IP ROUTING

# RIP Metric Policy

Metric Policy Timer

  This value defines the frequency at which the metrics are updated.
  Range: 0~999 seconds

Port

  This field enables you to select the port for which the metrics apply.
  Range: WAN, or LAN port

DLCI

  If the selected port is a WAN port, you may specify a particular DLCI for which the metrics apply.
  Range: 16~1023

Metric

  This is the way value you want to place on the specified route.
  Range: 0~15