  CONFIGURATION EDITOR
  MAPPINGS

# X.25 Pass-Through Mappings

Destination

Destination SAP

DLCI

ID

Increment DSAP

Increment SSAP

Far DTE Address

Frame Relay Port

Hunt Group

Near DTE Address

Source SAP

X.25 Port

  To add an entry, click on the Add button.
  To delete an entry, select it, then click on the Delete button.

ID

  This field defines the unit's mapping entry. This field increments automatically with each subsequent add.
  Range: 001 -- FFF

X.25 Port

  Click inside this field and select the port through which the X.25 traffic enters the unit.
  Range: 1 -- 8

Near DTE Address

  This is the address of your nearest PAD device. If the device does not appear in the list, you may add it though the Destination Editor.
  Range: Any device available in the pull-down list

Far DTE Address

  This is the address of your farthest PAD device on the opposite side of the frame relay. If the device does not appear in the list, you may add it though the Destination Editor.
  Range: Any device available in the pull-down list

Frame Relay Port

  Click on this field to select the appropriate frame relay port.
  Range: 1 --8

Destination

  Click on this field to select the appropriate destination from the pull-down list. If you do not see your destination, you may add it though the Destination Editor.
  Range: Any device available from the pull-down list

Destination SAP

  This field defines the SAP address of the destination device.
  Range: 04 -- FF (in increments of 4)

Source SAP

  This field defines the SAP address of the source device.
  Range: 04 -- FF (in increments of 4)

DLCI

  Enter the DLCI you want the unit to use for the specified frame relay port.
  Range: 16 -- 1023

Increment DSAP

  Select this option if you want the DSAP to increment automatically for every added entry. You may want to do this if your source stays the same for the added entries.
  Range: Enabled or Disabled

Increment SSAP

  Select this option if you want the SSAP to increment automatically for every added entry. You may want to do this if your destination stays the same for the added entries.
  Range: Enabled or Disabled

Hunt Group

  This feature enables you to use load leveling.