  EDITOR HOME
  UNIT LEVEL

# Passwords

  Confirm SNMP Get Community Name
  Confirm SNMP Set Community Name
  Confirm TFTP Download Password
  SNMP Get Community Name
  SNMP Set Community Name
  TFTP Download Password

  This screen enables you to configure passwords that allow access to various SNMP Get, Set, and TFTP file transfer commands.
  SNMP Get Community Name
  This alphanumeric password is used to authenticate MIB Get requests. The default name is "Public". Note that before clicking on the OK button, you must confirm the new Get Community Name password.
  Range: 0 ~ 15 alphanumeric characters
  Confirm SNMP Get Community Name
  This password must match the above password identically, as a confirmation. This field is case sensitive and must match exactly the new
  Range: 0 ~ 15 alphanumeric characters
  SNMP Set Community Name
  This alphanumeric password is used to authenticate SNMP Set requests. The default name is "Private".
  Range: 0 ~ 15 alphanumeric characters
  Confirm SNMP Set Community Name
  This password must match the above password identically, as a confirmation.
  Range: 0 ~ 15 alphanumeric characters
  TFTP Download Password
  This alphanumeric password enables the user to transfer files to and from the unit.
  Range: 0 ~ 8 alphanumeric characters
  Confirm TFTP Download Password
  This password must match the above password identically, as a confirmation.
  Range: 0 ~ 8 alphanumeric characters