# Unit Detail

# Unit Monitoring

# Displaying Network Port Statistics

#### Network Port Statistics

#### Port Statistics

#### Displaying Network Port Statistics

  The NET Port Statistics window provides the user with physical Layer 2 Throughput statistics collected on the Network interface.
  To open the NET Port Statistics window:
  1 Position the mouse arrow over the Unit Detail window's graphical representation of the Network port, and click the right mouse button.
  2 Select Port Statistics... from the list of pull-down menu options and click the left mouse button.
  Note: The Network statistics window can also be opened from the Network Port Status window. After opening the status window click on the Statistics...button. For information about the Network Port Status window, refer to "Displaying Network Status Information,"
  The fields and buttons contained within the NET Port Statistics window are described in the following paragraphs. The value displayed in parentheses represents the difference (delta) between values obtained during the previous polling interval and the current interval.
  Port Statistics - Identifies Layer 2 Throughput statistics collected on High-level Data Link Control (HDLC) frames passing through the Network interface port.

Network Port Statistics

  In Octets ~ The number of octets (bytes) which have been received on the Network interface.
  Out Octets ~ The number of octets (bytes) which have been transmitted on the Network interface.
  In Frames ~ The number of frames which have been received on the Network interface.
  Out Frames ~ The number of frames which have been transmitted on the Network interface.
  In CRC Errors ~ The number of frames which have been received on the Network interface. that contain Cyclic Redundancy Check (CRC) errors. The unit can be configured to either discard or pass through CRC errored frames..
  In Aborts ~ The number of frames which have been received on the Network interface. that have been marked with an abort sequence (indicates that the frames were incomplete).
  Stop/Start - Clicking this button stops and starts the statistics polling action.
  Update - Clicking this button will update (refresh) the counts of each Network interface Throughput statistic.
  Done - Clicking this button will close the NET Port Statistics window.