  CONFIGURATION EDITOR
  MAPPINGS
  X.25 PASS-THROUGH

# X.25 Pass-Through

# Hunt Group

  To add an entry, click on the Add button.
  To delete an entry, select it, then click on the Delete button.

ID

  This is the ID automatically given to the entry and cannot be changed.

Port

  This is the X.25 port you want included in the Hunt Group.
  Range: 1 -- 8

DTE Address

  This is the PAD device you want to include in the Hunt Group.
  Range: Any device listed in the pull-down list