  CONFIGURATION EDITOR
  FILTERING

# IP Filtering

  Note: Depending upon your product type, this dialog may vary. This help context covers all possible configuration parameters. If your dialog does not contain certain parameters, they don't apply to the product you are configuring.

Filter Out IP Frames

  Enable this option if you want to filter IP frames on all routes.

Virtual-Port Specific Filtering Overrides

  This feature enables you to specify filtering overrides for certain ports and DLCIs. These filters will override the default filter setting.
  1. Click on the Add button.
  2. Click inside the port field to select a port.
  3. Click inside the DLCI field and enter the provider-assigned DLCI number.
  4. Click inside the Filter Out IP Frames field to set the filtering to Yes or No.
  Range: Ports: 1 --8, DLCIs: 16 -- 1023, Filter Frames: Yes or No
  Also See Bridge Filtering