# Customize

  Connections enables you to define how the program handles connection attempts. These parameters work independently from the management protocol.
  FRAD/SNMP must be set if you intend to manage frads via SNMP.
  FRAP/SNMP must be set if you intend to manage frads via SNMP.
  IP/SNMP must be set if you intend to manage units via IP.
  LLC2 must be set if you intend to manage units via IP.
  Miscellaneous enables you to activate or deactivate global program features.
  Scheduler enables you to define limitations for the installation scheduler feature.
  Session Tuning enables you to define how many sessions the program can manage at a given time. These values can only be modified for LLC2.