Load On/Off and Input Terminal Setup

Load on/off

INP

Turns the load on or off.

Command

INPut[:STATe] {ON|OFF|1|0}

INPut[:STATe]?

Parameter

Value: | ON (1) | Load on
| OFF(0) | Load off (default)

Table 4 shows the setting that is specified when *RST is sent.

Response

Returns the load on/off state in the NR1 form in response to INP?.

INP:PROT:CLE

Clears the load input PROTECTION alarm.

Command

INPut:PROTection:CLEar