
QuadTech Incorporated

End-User License Agreement

1. 	Copyright:
	All copyrights to the programs and sources on this CD are
	the property of QuadTech, Inc..

2. 	Use of Software:
	The software is distributed "as is".  No warranty of any
   	kind is expressed or implied.  The End-User uses this
	software at his own risk.

3.	Liability:
	The author is not liable for data loss, damages, loss of
	profits or any other kind of loss that may be incurred
	while using or misusing this software.

4.	Installation:
	To install the software, open .zip and double-click on the setup icon.

5.	1900 Virtual Front Panel Operation

	This program allows configuration, measurements and data from the
	1910/20 to be saved to a file.  A measurement can be initiated from
	the software program.

	Set correct Com Port and Baud Rate, click "Finished"  
	Baud rate setting of 1910/20 can be found in Utility, RS-232 Baud Rate

6.	Result screen
	
   *    Log button will allow file to be opened. 
	You will be prompted to select or enter a file.
	If a file exists you will be asked if you want new data to
	overwrite or append to existing data in the file. 
 
   *    Configure button will open the configure screen
		A test and test conditions can be configured on the left side,
		use "Update Test" to send configuration to the 1910/20
 
		System conditions can be configured on the right side, use "Update
		Sys" to send configuration to the 1910/20

		Exit returns to the Results screen
		
   *    A measurement can be initiated by clicking the Start button.
	Measurements will also be saved if logging has been initiated
	
	Once data has been collected click "Stop Log" button to close
	file so it can be accessed by another program such as Excel.

   *    Clicking the "Not Locked Out" button will lock the front panel of the unit,
	clicking the "Locked Out" button will unlock the front panel of the unit
		
   
