ContentsPreviousNext
Settings

# Setting Up a Client Computer

Follow the procedure below to configure a computer as a client computer and connect it to the shared printer. Make this setting when installing the printer driver from the CD-ROM provided.

- For Windows 2000/XP, Windows Server 2003, and Windows NT 4.0, log on as an administrator (a user with an administrator right).

- Configure a computer connected to the network where the print server is connected.

Start Windows, and then insert the "Drivers & Manual" CD-ROM into the CD-ROM drive.

- Quit all other applications currently running.

- When starting Windows, a wizard for adding new hardware may open. If this happens, click [Cancel]. Check again that the power is off, and then proceed to step .

- When the CD-ROM is inserted, the [Drivers and Manual] dialog box appears. If it does not, double-click the CD-ROM drive icon under [My Computer] or [Explorer], and then double-click [SETUP.EXE].

Select a language for the interface, and then click [OK].

The following languages are available:

Deutsch (German), English (English), Espanol (Spanish), Francais (French), Italiano (Italian), Nederlands (Dutch) The default interface language is English.

Click [Printer Driver].

Read the license agreement, and then click [I accept the agreement.].

Click [Next >].

Click [Connected via LAN].

Click [Next >].

Click the plus mark next to a printer name.

Click [Port:] under [Printer Name:].

Click [Add].

The [Add Port] dialog box appears.

Click [Network Printer].

Click [OK].

Select a shared printer.

Click [OK].

Check that [<\\servername\sharedprintername>] appears after [Port:].

Installation starts.

Click [Finish].

Check the installation result, and then click [Finish].

- If the message prompting you to restart the computer appears, restart the computer.

- For details about installing the printer driver, see "Installing the Printer Driver", the Setup Guide.

- Setting Up a Server