| ContentsPreviousNext |

# Paper Size Mismatch (Bypass Tray)

Paper of the incorrect size is loaded. Follow the procedure below to load the correct size of paper or change the paper size in the printer properties settings.

1. Open the printer properties dialog box from the application.

2. Click the [Page Settings] tab.

3. In the [Original size:] and [Printout paper size:] lists, check document and paper sizes. To change the paper size, select a paper size in the [Printout paper size:] list.

   To enable the [Printout paper size:] list, select the [Reduce/Enlarge] check box.

   - If incorrect document and paper sizes are selected in the [Original size:] and [Printout paper size:] lists, cancel printing, and then select the correct sizes.

   - If paper of the incorrect size is loaded, proceed to the next step.

4. Slide the bypass tray guides into position according to the paper size.

5. Insert a sheet of paper into the bypass tray with the print side face up.

   - Support the sheet with your hands to keep it from sliding out and dropping.

   - Insert the sheet straight into the bypass tray.

6. Press the [Test Paper Feed/Resume] key, and then push the sheet into the printer a little.

   Printing starts.

- Opening from an Application

- Canceling Printing