ContentsPreviousNext
Settings

# Nozzle Check

Follow the procedure below to check whether the print-head nozzles are clogged up or not by printing a nozzle check test pattern.

- To check the printed test pattern, proceed to step 7..

1. Open the printer properties dialog box.

2. Click the [Maintenance] tab.

3. Click [Nozzle Check].

4. Click [Next >].

5. Check that A4/Letter size paper is loaded in the paper tray.

6. Click [Next >].

7. Check the printed test pattern.

   Normal

   When print-heads are clogged

8. Click [Finish].

   - If the printed test pattern is not clear, select the [Clean print-heads (normal)] check box, and then click [Next >].

- Opening from the Start Menu

- Opening from an Application

- Clean Print-heads (Normal)