ContentsPreviousNext
Settings

# Printer Body

Print speed

Measurements according to the manufacturer's measurement system

Black draft: 19 ppm

Black standard (speed priority): 12 ppm

Color draft: 19 ppm

Color standard (speed priority): 12 ppm

Depending on the operating environment, printing may take longer than normal.

Print direction

Supports bidirectional, minimum distance printing

Print resolution

Max 3600 × 1200 dpi equivalent

Nozzles

Black: 192 nozzles

Cyan, magenta, and yellow: 192 nozzles per color

Paper sizes (Tray 1 : standard)

A4 (portrait), B5 (portrait), A5 (landscape), A6 (portrait), Legal (portrait), Letter (portrait), 5 1/2"×8 1/2" (landscape), Exective (portrait) (184.2 mm × 266.7 mm (7.3 × 10.5 inches)), F (portrait) (203.2 mm × 330.2 mm (8.0 × 13.0 inches)), Foolscap (F4) (portrait) (215.9 mm × 330.2 mm (8.5 × 13.0 inches)), Folio (portrait) (209.5 mm × 330.2 mm (8.3 × 13.0 inches)),

Custom paper sizes: 148-356 mm (length) × 90-216 mm (width), (5.9-14.1 inches (length) × 3.6-8.5 inches (width))

Paper sizes (Bypass tray)

Standard paper size: A4 (portrait), B5 (portrait), A5 (landscape), A6 (portrait), Legal (portrait), Letter (portrait), 5 1/2"×8 1/2" (landscape), Exective (portrait) (184.2 mm × 266.7 mm (7.3 × 10.5 inches)), F (portrait) (203.2 mm × 330.2 mm (8.0 × 13.0 inches)), Foolscap (F4) (portrait) (215.9 mm × 330.2 mm (8.5 × 13.0 inches)), Folio (portrait) (209.5 mm × 330.2 mm (8.3 × 13.0 inches)), Com10 (portrait) (104.8 mm × 241.3 mm (4.2 × 9.5 inches)), Monarch (portrait) (98.4 mm × 190.5 mm (3.9 × 7.5 inches)), C6 (portrait) (114 mm × 162 mm (4.5 × 6.4 inches)), C5 (portrait) (162 mm × 229 mm (6.4 × 9.1 inches)), DL Env (portrait) (110 mm × 220 mm (4.4 × 8.7 inches))

Custom paper sizes: 148-1295.4 mm (length) × 90-216 mm (width), (5.9-51.0 inches (length) × 3.6-8.5 inches (width))

Paper type

Plain paper

Recycled paper

Color paper

Inkjet plain paper

Semi-gloss photo paper

Inkjet transparency

Paper weight

Tray 1/optional tray: 60-105 g/m2 (114.7-198.5 lb.)

Bypass tray: 60-163 g/m2 (114.7-297.7 lb.)

Maximum paper capacity

Tray 1: 200 sheets

Bypass tray: 1 sheet

Output tray capacity

150 sheets

The capacity may be less depending on the images printed.

Power supply

220-240 V, 0.3 A, 50/60 Hz (when fully equipped)

Power consumption

Average power consumption while printing: 27 W or less

Energy Saver mode: less than 6 W

When power is off: 0.3 W or less

To avoid any power consumption, disconnect the power plug from the wall outlet.

(Disconnect the power plug after turning the power off with the [Power] key.)

Operating environment

Temperature: 10 to 32°C (50 to 89.6°F)

Humidity: 15-80% RH (maximum wet-bulb temperature: 25°C (77°F) )

Printing may stop to protect the printer for conditions outside those described above.

Storage environment

Temperature: -20 to 43°C (-4 to 109.4°F)

Humidity: 15-80% RH

External dimensions

(W × D × H) 403 × 440 × 218 mm (15.9 × 17.4 × 8.6 inches)

Weight

Approximately 10 kg (22.1 lb.) (printer body with consumables)

Noise emission

Approximately 45 dB (high quality mode)

Interface

USB2.0 High Speed

Printer language

RPCS Raster

Print cartridges

Types and yields measured using A4 (Letter) 5% chart printed in standard (speed priority) mode.

Print cartridge black: approximately 1450 sheets

Print cartridge cyan: approximately 1000 sheets

Print cartridge magenta: approximately 1150 sheets

Print cartridge yellow: approximately 1150 sheets

The printing yields of Print cartridges vary depending on the number of times head cleaning is performed.Also, the printing yields of the Print cartridges packaged with the printer are lower than the yields of the Print cartridges available for purchase separately.