ContentsPreviousNext
Settings

# Printable Area

Printable and unprintable areas

1. Feed Direction

2. Printable Area

3. 3 mm (0.12 inches)

- Do not attempt to print beyond the guaranteed printable area. Paper feed precision is reduced around the printable area limits, resulting in lower print quality.

- When printing on envelopes, the following print area limitations apply.

1. Feed Direction

2. Printable Area

3. 8 mm (0.4 inches)

4. 38 mm (1.5 inches)

5. 5 mm (0.2 inches)