ContentsPreviousNext
Settings

# Replacing a Print Cartridge

Follow the procedure below to replace an empty Print cartridge.

Clear any errors, such as when there is a paper jam or when no paper is loaded, before replacing a Print cartridge.

Remove the Print cartridges' packaging.

- If multiple cartridges are empty, replace all the empty cartridges. You can shorten the time for needed replacement.

Open the right front cover.

Take out the empty cartridges.

Check the cartridges' orientation, and then install them gently.

Install in the following order from the left: black, cyan, magenta, and yellow.

- Take care to install the cartridges in the correct position.

Push in the cartridge using the PUSH area.

Close the right front cover.

- Recommended Consumables