ContentsPreviousNext
Settings

# Removing Paper Jammed in the Paper Tray

Follow the procedure below to remove paper jammed in the paper tray.

Lift the output tray.

When the output tray is lifted, the paper tray will pop out slightly.

Hold both sides of the paper tray, and then pull it toward you.

- The paper tray cannot be detached. Do not pull it forcefully.

Remove jammed paper.

- If you cannot remove the jammed paper or it is difficult to remove, the paper may be jammed inside the printer. Examine the paper carefully and remove.

- If you cannot locate jammed paper, it may be jammed inside the printer.

Hold both sides of the paper tray, and push it gently in until it stops.

Lower the output tray.

Press the [Test Paper Feed/Resume] key.

Printing starts.

- Blank paper may be delivered after printing resumes.

- Removing Paper Jammed around the Guide Board

- Paper Is Not Fed or Delivered Normally