| ContentsPreviousNext |

# Removing Paper Jammed in the Duplex Unit (optional)

Follow the procedure below to remove paper jammed in the duplex unit (optional).

1. Press the duplex unit cover button, and then open the duplex unit.

2. Remove jammed paper.

3. Close the duplex unit cover.

4. Press the [Test Paper Feed/Resume] key.

   Printing starts.

   - Depending on how the paper was jammed, printing may resume from the next page, not the one jammed