| ContentsPreviousNext |

# Non-compatible Paper

Check if the paper is compatible.

Do not use paper that is:

- wrinkled, folded, or damaged

- wavy at the ends

- curled

- absorbent

- dry and conducive to static buildup

- already printed on

- preprinted (unless specified)

- heat sensitive/non-carbon

- too thick or thin

- pre-stitched or hole-punched

- glued or tacked

- stapled or clipped together

- dark in places

- irregular in length and proportion

- Even if compatible paper types are used, print quality may be lower than usual or paper jams may occur if the paper was improperly stored.