| ContentsPreviousNext |

# Paper Will Not Feed Even When the Power Is On

If printing will not start even when the power is on, check if an error has occurred using the indicators or Printer Status monitor.

An indicator is lit or blinking

Only the [Power] key is blinking.

The printer may be receiving data or replenishing its ink. Wait momentarily for the blinking [Power] key to stop and stay lit.

The [Test Paper Feed/Resume] key or a low ink indicator is blinking or lit.

An error has occurred. See Error Indicator Summary.

An error message is displayed on the Printer Status monitor.

Click [User Guide...] to display the page corresponding to the error where you can check how to solve the problem in more detail. See Printer Status Monitor Errors.

A print sample can be printed using keys on the control panel to check that the printer is not out of order.

When the power is off, while holding down the [Cancel] key and the [Test Paper Feed/Resume] key, press and hold down the [Power] key for over three seconds. The low ink indicators will light once and a print sample will be delivered.