| ContentsPreviousNext |

# Paper Is Not Fed or Delivered Normally

If the printer is operating but paper will not feed or paper jams multiple times, check the condition of the printer and paper.

Paper does not feed smoothly.

Paper guides are not adjusted properly.

- The paper guides of the paper tray do not match the paper loaded. Adjust the paper guides and load the paper again. See Loading Paper.

Paper is not loaded properly.

- The paper is not loaded properly. Load the paper correctly. See Loading Paper.

Paper is curled.

- Remove the loaded paper and check if it is curled. If it is, straighten the curl.

Paper that is not compatible is loaded.

- Remove the loaded paper and replace it with compatible paper. See Non-compatible Paper.

Paper jams multiple times.

The guide board is not closed.

- Make sure that the guide board is closed. Remove the rear cover and press both sides of the guide board until it clicks closed.

Multiple sheets are inserted in the bypass tray.

- When using the bypass tray, insert paper one sheet at a time. See Printing on Thick Paper.

Printing densely colored images on both sides.

- When printing images containing areas of solid color that consume a lot of ink, we recommend single-sided printing.

Multiple sheets of paper are fed at one time.

Load the paper again. Remove the paper from the paper tray, fan it well, and tap it on a flat surface such as a desk to even the edges. Check the position of the paper guides of the paper tray, and then load the paper again.

Though a paper jam is cleared, paper does not feed.

When a paper jam occurs, clear the paper jam, and then press the [Test Paper Feed/Resume] key. See Paper Jam.

- If an error is displayed on the Printer Status monitor, follow the instructions to solve the problem. See Printer Status Monitor Errors.