TG700 Signal Download Files
14-August-2000


Signals Contained in Each Download File
---------------------------------------
Module:         DVG7
File name:      525-1431.DNL	Size:   394.7k

Signal Set      Button Name     Signals
---------       -----------     -------

525-143		COLOR BAR       100%^Color Bars
				75%^Color Bars
				SMPTE^Color Bars

		FLAT FIELD      0%^Flat Field
				100%^Flat Field
				50%^Flat Field
				Black^Burst
				Field^Square Wave

		LINEARITY       10 Step
				5 Step
				Luminance^Ramp
				Mod Shallow^Ramp
				Modulated^10 Step
				Modulated^5 Step
				Modulated^Pedestal
				Modulated^Ramp
				Shallow^Ramp
				Shallow^Ramp Matrix

		MONITOR         100% Red^Field
				2 Level^Ped. & Pluge
				4 Level^Ped. & Pluge
				75% Red^Field
				Convergence^Pattern
				Grey^Window
				Monitor^Matrix
				Monitor^Setup
				White^Window

		MULTIBURST	60 IRE^Multiburst
				Multipulse

		SWEEP		6 MHz^Sweep
				SinX/X

		SDI		Equalizer^Test
				PLL Test
				SDI^Matrix

		PULSE BAR	Window 1T^Pulse & Bar
				Window 2T^Pulse & Bar

		OTHER           FCC^Componsite
				FCC^Multiburst
				NTC7^Combination
				NTC7^Composite
	
		APL		FCC^Composite^High APL
				FCC^Composite^Low APL
				Mod 5 Step^High APL
				Mod 5 Step^Low APL
				Mod Ramp^High APL
				Mod Ramp^Low APL
				NTC7^Combination^High APL
				NTC7^Combination^Low APL
				NTC7^Composite^High APL
				NTC7^Composite^Low APL

		COLOR BAR	100%^Color Bars
		No Setup	75%^Color Bars
				SMPTE^Color Bars	
		
-------------------------------------------------------
Module:         DVG7
File name:      525-270.DNL	Size:   221.5K

Signal Set      Button Name     Signals
---------       -----------     -------

525-270		COLOR BAR       100%^Color Bars
				75%^Color Bars
				SMPTE^Color Bars

		FLAT FIELD      0%^Flat Field
				100%^Flat Field
				50%^Flat Field
				Field^Square Wave

		LINEARITY       10 Step
				3 Channel^Ramp
				5 Step
				B-Y^Valid Ramp
				Limit^Ramp
				Modulated^Ramp
				Oversize^Ramp
				R-Y^Valid Ramp
				Shallow^Ramp
				Shallow^Ramp^Matrix
				Valid^Ramp
				Y^Valid Ramp
		
		MONITOR         2 Level^Ped. & Pluge
				4 Level^Ped. & Pluge
				75% Red^Field
				75% Green^Field
				75% Blue^Field
				Convergence^Pattern
				Gamut Test
				Grey^Window
				White^Window

		MULTIBURST	60%^Multiburst
				Multipulse

		SWEEP		100% Sweep
				60%^Sweep
				SinX/X
				
		SDI		Equalizer^Test
				PLL Test
				SDI^Matrix

		TIMING		2.5 MHz^Bowtie
				500 KHz^Bowtie
				Active^Picture^Timing
				Co-siting^Pulse

		PULSE BAR	2T^Pulse & Bar
				T Pulses

		OTHER		Chroma^Freq. Resp.
				Color^Palette
				FCC^Composite
				FCC^Multiburst
				NTC7^Combination
				NTC7^Composite

-------------------------------------------------------
Module:         DVG7
File name:      625-270.DNL	Size:   200.9K

Signal Set      Button Name     Signals
---------       -----------     -------

625-270		COLOR BAR       100%^Colour Bars
				75%^Colour Bars
				100%^Colour Bars^Over Red
				75%^Colour Bars^Over Red

		FLAT FIELD      0%^Flat Field
				100%^Flat Field
				50%^Flat Field
				Field^Square Wave

		LINEARITY       10 Step
				3 Channel^Ramp
				5 Step
				B-Y^Valid Ramp
				Limit^Ramp
				Modulated^Ramp
				Oversize^Ramp
				R-Y^Valid Ramp
				Shallow^Ramp
				Shallow^Ramp^Matrix
				Y^Valid Ramp
		
		MONITOR         100% Red^Field
				2 Level^Ped. & Pluge
				4 Level^Ped. & Pluge
				75% Red^Field
				Convergence^Pattern
				Gamut Test
				Grey^Window
				White^Window
				
		MULTIBURST	60%^Multiburst

		SWEEP		100% Sweep
				60%^Sweep
				SinX/X

		SDI		Equalizer^Test
				PLL Test
				SDI^Matrix

		TIMING		2.5 MHz^Bowtie
				500 KHz^Bowtie
				Active^Picture^Timing
				Co-siting^Pulse
				
		PULSE BAR	2T 4T 10T^Pulse & Bar
				2T 4T 20T^Pulse & Bar

		OTHER		CCIR 17
				CCIR 18
				CCIR 330
				CCIR 331
				CCIR 331^G2

------------------------------------------------------------
