TG700 Signal Download Files
20-April-2002


Signals Contained in Each Download File
---------------------------------------
Module:         ATG7
File name:      NTSC.DNL	Size:   256 k

Signal Set      Button Name     Signals
---------       -----------     -------
NTSC		COLOR BAR	100% Colour Bars
				75% Colour Bars
				SMPTE Colour Bars

		LINEARITY	10 Step
				5 Step
				Modulated 5 Step
				Modulared Pedestal
				Modulated Ramp
				Ramp
				Shallow Ramp

		FLAT FIELD	0% Flat Field
				10% Flat Field
				100% Flat Field
				40% Flat Field
				50% Flat Field
				Black Burst
				Black Burst with Field Ref
				Field Square Wave

		MULTIBURST	100% Multiburst
				60% Multiburst
				Multipulse

		MONITOR		100% Red Field
				2 Level Pedestal & Pluge
				4 Level Pedestal & Pluge
				75% Red Field
				Convergence Pattern
				Gray Window
				Monitor Setup
				Safe Area
				White Window

		SWEEP		100% Sweep
				60% Sweep
				Chroma Frequency Response

		PULSE BAR	Sin X/X
				Window 2T Pulse & Bar

		OTHER		FCC Composite
				FCC Multiburst
				Matrix 1
				NTC7 Combination
				NTC7 Composite
				SNG Color Bars

---------
NTSC		BARS Output	100% Colour Bar
				75% Colour Bar
				SMPTE Colour Bar
				40% Flat Field
				Black Burst
				Black Burst with Field Ref
				Other 1
				Other 2

-------------------------------------------------------
Module:         ATG7
File name:      NTSC_NSU.DNL	Size:   239 k

Signal Set      Button Name     Signals
---------       -----------     -------
NTSC No Setup	COLOR BAR	100% Colour Bars
				75% Colour Bars
				SMPTE Colour Bars

		LINEARITY	10 Step
				5 Step
				Modulated 5 Step
				Modulared Pedestal
				Modulated Ramp
				Ramp
				Shallow Ramp

		FLAT FIELD	10% Flat Field
				100% Flat Field
				40% Flat Field
				50% Flat Field
				Black Burst
				Black Burst with Field Ref
				Field Square Wave

		MULTIBURST	100% Multiburst
				60% Multiburst
				Multipulse

		MONITOR		100% Red Field
				2 Level Pedestal & Pluge
				4 Level Pedestal & Pluge
				75% Red Field
				Convergence Pattern
				Gray Window
				Monitor Setup
				Safe Area
				White Window

		SWEEP		100% Sweep
				60% Sweep
				Chroma Frequency Response

		PULSE BAR	Sin X/X
				Window 2T Pulse & Bar

		OTHER		FCC Composite
				FCC Multiburst
				Matrix 1
				NTC7 Combination
				NTC7 Composite
				SNG Color Bars

---------
NTSC No Setup	BARS Output	100% Colour Bar
				75% Colour Bar
				SMPTE Colour Bar
				40% Flat Field
				Black Burst
				Black Burst with Field Ref
				Other 1
				Other 2

-------------------------------------------------------
Module:         ATG7
File name:      PAL.DNL		Size:   362 k

Signal Set      Button Name     Signals
---------       -----------     -------
PAL		COLOR BAR	100% Colour Bars
				100% Colour Bars Over Red
				75% Colour Bars
				75% Colour Bars Over Red

		FLAT FIELD	100% Flat Field
				40% Flat Field
				50% Flat Field
				Black Burst
				Black Burst with No Field Ref
				Field Square Wave

		LINEARITY	10 Step
				5 Step
				Modulated 10 Step
				Modulated 5 Step
				Modulared Pedestal
				Modulated Ramp
				Ramp
				Shallow Ramp

		MONITOR		100% Red Field
				2 Level Pedestal & Pluge
				4 Level Pedestal & Pluge
				75% Red Field
				Convergence Pattern
				Grey Window
				Monitor Setup Matrix
				Safe Area
				White Window

		MULTIBURST	100% Multiburst
				Multipulse

		SWEEP		100% Sweep
				60% Sweep

		PULSE BAR	Sin X/X
				Window 2T Pulse & Bar

		OTHER		CCIR 17
				CCIR 18
				CCIR 330
				CCIR 331
				ITS Matrix 1
				UK 1 Line ITS
				UK ITS 1
				UK ITS 2
	
---------
PAL		BARS Output	100% Colour Bar
				75% Colour Bar
				100% Colour Bar	Over Red
				75% Colour Bar Over Red
				40% Flat Field
				Black Burst
				Black Burst No Field Ref
				Other 1
				Other 2

------------------------------------------------------------
