Maintain an M9 Pistol Reviews
Summary Lubricate the Pistol and Magazine
24 of 35
&pageText=To correctly lubricate the M9 pistol and magazine, you must:& &bulletText1= Lubricate the slide assembly, both inside and
outside, and make sure to lubricate the safety.& &bulletText2= Lubricate the barrel assembly, the locking
block plunger, and the locking lugs.& &bulletText3= Lubricate the recoil spring and recoil
spring guide.& &bulletText4= Lubricate the receiver assembly, to include
the slide stop, magazine stop, and the
guide rails.& &bulletText5= Lubricate the magazine tube, spring, follower,
floorplate retainer, and floorplate.&