Maintain an M9 Pistol Exercises
Practical Exercise
2 of 14
&pageText=Scenario: You’ve completed a live-fire training exercise with your assigned pistol. Now you need to perform maintenance on your M9 pistol.
To maintain the M9 pistol, you need to complete the following performance measures in the correct order.& &label1=Clear the pistol.& &label2=Disassemble the pistol and magazine.& &label3=Clean the pistol, components, and ammunition.& &label4=Inspect the pistol, components, and ammunition.& &label5=Lubricate the pistol and magazine.& &label6=Assemble the pistol and magazine.& &label7=Perform a function check.& &link1=b385p0030.html& &link2=b385p0040.html& &link3=b385p0060.html& &link4=b385p0080.html& &link5=b385p0090.html& &link6=b385p0100.html& &link7=b385p0120.html& &instrucText=Follow these instructions:
1. Click the performance measure buttons in order to indicate the correct sequence. Begin by clicking the first step in the process. A number will appear in the box next to the button to help you remember the order you indicated.
2. When you click a button, you will go to another screen to complete an exercise on that step.
3. After you complete the exercise, you will return to this screen. At that point, you must click the next step in the process.
4. Continue until you have completed exercises on each performance measure.&