Maintain an M9 Pistol Reviews
Perform a Function Check
31 of 35
&pageText=To perform a function check on the M9 pistol, you must correctly perform the following procedures:& &textLabel1=Clear the pistol& &textLabel2=Depress the slide stop and let the slide go forward& &textLabel3=Insert an empty magazine into the pistol& &textLabel4=Retract the slide fully and then release it& &textLabel5=Depress the magazine release button and remove the magazine& &textLabel6=Place the safety lever in the SAFE position& &textLabel7=Depress the slide stop and let the slide go forward& &textLabel8=Squeeze and release the trigger& &textLabel9=Place the safety lever in the FIRE position& &textLabel10=Squeeze the trigger& &textLabel11=Squeeze trigger and hold to rear while retracting and releasing slide and then release trigger& &textLabel12=Squeeze the trigger again& &textPosition=left& &mediaStyle=swf& &imageBorder=true& &enableBtns=audio&