Maintain an M240B Machine Gun Reviews
Clean the Receiver
16 of 55
&pageText=To properly clean the receiver, you must:& &label1=Use chamber brush and CLP& &label2=Swab chamber with cleaning patches and CLP& &label3=Swab chamber with dry cleaning patches& &label4=Use receiver brush and CLP& &label5=Swab receiver with cleaning patches and CLP& &label6=Swab receiver with dry cleaning patches& &popText1=Apply CLP to the chamber brush and insert it into the chamber, twisting several times to remove powder fouling and other foreign matter.& &popText2=Swab the chamber using cleaning patches dampened with CLP.& &popText3=Then swab the chamber again with dry cleaning patches.& &popText4=Clean the receiver using a receiver brush and CLP to remove powder fouling and other foreign matter. & &popText5=Swab the receiver using cleaning patches dampened with CLP.& &popText6=Swab the receiver using dry cleaning patches to remove all traces of foreign matter and CLP.&