Maintain an M240B Machine Gun Reviews
Inspect the Bolt and Operating Rod Assembly
29 of 55
&pageText=To properly inspect the bolt and operating rod assembly, you must check:& &label1=Bolt and operating rod assembly& &label2=Firing pin& &label3=Extractor& &poptext1=Inspect entire assembly for bent, broken, cracked, or missing parts. Check surface for burrs or pits.& &poptext2=Check for cracks or wear on tip of firing pin.& &poptext3=Ensure you cannot move extractor with finger pressure.&