Maintain an M240B Machine Gun Reviews
Inspect the Butt Stock and Buffer Assembly
27 of 55
&pageText=To properly inspect the butt stock and buffer assembly, you must check:& &label1=Mating grooves and flanges& &label2=Backplate latch& &label3=Buffer plug& &label4=Buffer& &label5=Butt stock& &poptext1=Check for burrs and rough edges on mating grooves and flanges.& &poptext2=Check backplate latch to ensure it locks buffer assembly securely to receiver.& &poptext3=Check buffer plug and ensure it sticks out through backplate and is flush or higher than protrusion below it.& &poptext4=Check buffer for rattling sounds. Ensure plug cannot rotate by finger pressure.& &poptext5=Check butt stock for cracks.&