Maintain an M240B Machine Gun Reviews
Inspect the Cover Assembly
31 of 55
&pageText=To properly inspect the cover assembly, you must check:& &label1=Feed lever& &label2=Cover latches and retaining clip& &label3=Cartridge guides and feed pawls& &label4=Accessory-mounting rails& &poptext1=Pivot feed lever back and forth to ensure it operates smoothly without binding.& &poptext2=Push in on cover latches to ensure retaining clip is present, secure, and does not bind.& &poptext3=Push down on cartridge guides and feed pawls to ensure springs are present and secure.& &poptext4=Inspect accessory-mounting rail for nicks or burrs.&