Maintain an M240B Machine Gun Reviews
Inspect the Trigger-Housing Assembly
30 of 55
&pageText=To properly inspect the trigger-housing assembly, you must check:& &label1=Assembly parts& &label2=Tripping lever and sear& &label3=Cocking action& &label4=Safety& &poptext1=Check for broken, missing, or damaged parts including sear spring, grip assembly, trigger guard, and trigger spring pin.& &poptext2=Inspect tripping lever and sear for burrs on edges.& &poptext3=Check cocking action by pushing back on tripping lever to ensure sear rises, and pulling trigger to ensure sear lowers.& &poptext4=Place safety on SAFE and pull trigger. Sear should not lock in downward position. Place safety on FIRE and pull trigger. The sear should drop down and lock in downward position.&