Maintain an M240B Machine Gun Reviews
Quick Review 6
41 of 55
&questionText=Determine the correct answer to the question and indicate your answer by clicking the letter next to your choice.
Which of the following is the preferred method of lubricating the M240B machine gun’s tripod mount components (tripod, Traversing and Elevating mechanism, and gun cradle mount)?& &lure1=Generous lubrication on all moveable parts& &lure2=Light lubrication on all moveable parts& &lure3=Light lubrication, wipe with a rag to remove
excess oil& &lure4=These components should not be lubricated& &correctResponse=3& &attempts=2& &correctFeedback=Nice work. You correctly identified the proper method of lubricating the tripod mount components.& &correctFeedback2=Nice work. You correctly identified the proper method of lubricating the tripod mount components.& &incorrectFeedback1=That is incorrect. Consider the remaining choices and try again.& &failedFeedback=That is still incorrect. The proper method for cleaning the M240B’s tripod mount components is to lightly lubricate all the components and then remove excess oil with a rag.& &link=a395p0270.html& &mediaStyle=swf& &imageXpos=400& &imageYpos=120&