Maintain an M240B Machine Gun Reviews
Summary – Ensure Weapon is Clear
8 of 55
&pageText=You should now be comfortable with the process for ensuring the M240B is clear. This is crucial, as ammunition left in the chamber may accidentally detonate during disassembly or cleaning. To clear the M240B, you must:& &bulletText1=Switch the safety to FIRE& &bulletText2=Pull cocking handle to the rear, and return to forward position& &bulletText3=Switch the safety to SAFE& &bulletText4=Open cover, and inspect chamber& &bulletText5=Lower feed tray& &bulletText6=Switch the safety to FIRE& &bulletText7=Ride the bolt forward& &bulletText8=Close cover&