Maintain an M240B Machine Gun Reviews
Replace the Trigger-Housing Assembly
46 of 55
&pageText=To properly replace the trigger-housing assembly, you must:& &label1=Insert trigger-housing& &label2=Align holes& &label3=Insert spring pin& &poptext1=Insert holding notch on front of trigger-housing mechanism into forward recess on bottom of receiver.& &poptext2=Rotate rear of trigger-housing upwards and align holes with receiver mounting bracket.& &poptext3=Hold trigger-housing assembly in place and insert spring pin into hole to secure assembly to receiver.&